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KEY PROJECT INFORMATION
Key Project Information
	GS ID (s) of Project (s)
	GS11336

	Title of the project (s) covered by monitoring report
	Shuangbaotai Animal Manure Management System GHG Mitigation Project in Guangxi Province

	Version number of the PDD/VPA-DD (s) applicable to this monitoring report
	04

	Version number of the monitoring report
	03

	Completion date of the monitoring report 
	13/09/2022

	Date of project design certification
	05/09/2022

	Date of Last Annual Report
	NA

	Monitoring period number 
	01

	Duration of this monitoring period 
	The 1st monitoring period from 20/01/2021 to 31/03/2022 (first and last days included)

	Project Representative 
	The official focal point and project developer: Profit Carbon Environmental Energy Technology (Shanghai) Co., Ltd.
The project owner: Shuangbaotai Animal Husbandry Group Co., Ltd.

	Host Country
	People’s Republic of China

	Activity Requirements applied

	[bookmark: Check7]|X| Community Services Activities 
|_| Renewable Energy Activities 
|_| Land Use and Forestry Activities/Risks & Capacities 
|_| N/A 

	Methodology (ies) applied and version number
	[bookmark: OLE_LINK18]ACM0010 GHG emission reductions from manure management systems (Version 08.0)

	Product Requirements applied
	[bookmark: Check4]|X| GHG Emissions Reduction & Sequestration 
|_| Renewable Energy Label 
|_| N/A 


Table 1 - Sustainable Development Contributions Achieved
	Sustainable Development Goals Targeted
	SDG Impact 
	Amount Achieved
	Units/ Products

	SDG 13: Climate Action
	Amount of GHGs emission avoided or sequestered
	260,692
	tCO2e

	SDG 7: Affordable and Clean Energy
	Total electricity produced
	33,628.11
	MWh

	SDG 8: Decent Work and Economic Growth
	Total number of jobs
	18 full-time jobs created (including 9 females and 9 males)


Table 2 – Product Vintages

	SDG 7 Affordable and Clean Energy
	Amount Achieved

	Start Dates
	End Dates
	Total electricity produced (MWh)

	20/01/2021
	31/12/2021
	26,683.22  

	01/01/2022
	31/03/2022
	6,944.89

	20/01/2021
	31/03/2022
	33,628.11



	SDG 8 Decent Work and Economic Growth
	Amount Achieved

	Start Dates
	End Dates
	Total number of jobs

	20/01/2021
	31/12/2021
	18 full time jobs created, including 9 females and 9 males

	01/01/2022
	31/03/2022
	18 full time jobs created, including 9 females and 9 males

	20/01/2021
	31/03/2022
	18 full time jobs created, including 9 females and 9 males



	SDG 13 Climate Action
	Amount Achieved

	Start Dates
	End Dates
	Amount of GHGs emission avoided or sequestered (tCO2e)

	20/01/2021
	31/12/2021
	206,817

	01/01/2022
	31/03/2022
	53,875 

	20/01/2021
	31/03/2022
	260,692 
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SECTION A. [bookmark: _Ref49860651] DESCRIPTION OF PROJECT
[bookmark: _Toc40962734]General description of project 
>>
The project installs 9 sets of Animal Waste Management Systems (AWMSs) in 9 existing swine farms in Guangxi Zhuang Autonomous Region. The purpose of the project activity is to treat the manure and wastewater from the 9 swine farms to avoid methane emissions. 

The scenario prior to the implementation of the proposed project activity is that the manure and wastewater from the 9 swine farms were treated in uncovered anaerobic lagoons. 

[bookmark: _Hlk86257092][bookmark: _Hlk86259381]The project activity replaces the current open anaerobic lagoons with new AWMSs, and Each subsidiary swine farm installs one AWMS. All the manure and wastewater are collected and then be separated first. The separated solid are treated in aerobic composting system and the organic fertilizers are produced. Part of the fertilizer is supplied to the farmers living around for free and the others is be sold to the market. The separated liquid is treated through anaerobic digestion process and the biogas generated during the treatment process is captured for electricity generation and surplus biogas is destroyed through the flaring system (if any). The electricity generated are all used by the operation of AWMSs and the swine farms. It is estimated that total 25,859,844.12m3 biogas are expected to be generated annually and all of the biogas will be sent to biogas generator for power generation after desulfurization purification system. Each generator is installed in each subsidiary swine farm, total installed capacity of the proposed project is 5.2MW and the annual electricity production is estimated to be 33,100.60MWh. After anaerobic digestion. The sludge produced from anaerobic digestion are treated through aerobic composting together with the separated solid, the effluent is supplied to the farmers living around free for agriculture irrigation.

The project activity reduces GHG in the atmosphere through avoiding methane emissions from anaerobic treatment of swine manure and wastewater. The annual average CO2 emission reductions are estimated to be 267,474 tCO2e as per PDD.

The project has been put into operation in 20/01/2021. This monitoring report is for the 1st monitoring period, which is from 20/01/2021 to 31/03/2022. Total emission reductions achieved in this monitoring period are 260,692tCO2e.

[bookmark: _Toc40962735]Location of project 
>>
The proposed project activity is located in Guangxi Zhuang Autonomous Region, China. There are nine subsidiary farms involved in the project. Of which, there are one fatting farm: Debao Chengguan swine Farm, eight swine farm including market swine and breeding swine: Bama Yanyan swine Farm, Chongzuo Zuozhou swine Farm, Tianyang Wucun swine Farm, Quanzhou Dengjiabu swine Farm, Chongzuo Quming swine Farm, Jingxi swine Farm, Liucheng Mashan swine Farm and Tengxian Tianping swine Farm. The specific location of the nine subsidiary farms is shown below:
Table1. the specific location of the nine swine farms
	Swine Farm
	Location
	East longitude
	North latitude

	Bama Yanyan swine farm （巴马延岩猪场）
	Bama County, Hechi City
	107.231670544°
	23.976710754°

	Chongzuo Zuozhou swine Farm （崇左左州猪场）
	Zuozhou Town, Jiangzhou District, Chongzuo City
	107.456162364°
	22.648337404°

	Tianyang Wucun swine Farm （田阳五村猪场）
	Wucun Town, Tianyang District, Baise City
	106.800232°
	23.501188°

	Quanzhou Dengjiabu swine Farm （全州邓家埠猪场）
	Dengjiabu Village, Quanzhou County, Guilin City
	111.100142756°
	25.891490360°

	Chongzuo Quming swine Farm （崇左渠茗猪场）
	Quming Village, Fusui County, Chongzuo City
	107.456200450°
	22.686794907°

	Jingxi swine Farm （靖西猪场）
	Jingxi City
	106.315845°
	23.148953°

	Liucheng Mashan swine Farm （柳城马山猪场）
	Mashan Town, Liucheng County, Liuzhou City
	108.054611695°
	23.755085410°

	Tengxian Tianping swine Farm （藤县天平猪场）
	Tianping Town, Teng County, Wuzhou City
	110.773228845°
	23.375143765°

	Debao Chengguan swine Farm （德保城关猪场）
	Chenguan Town, Debao County, Baise City
	106.654436049°
	23.301572413°
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Figure 1 The Geographic Location of the project

[bookmark: _Toc40962736]Reference of applied methodology 
>>
The approved methodology applied by this project is referenced as ACM0010” GHG emission reductions from manure management systems (Version 08.0)”. 

Tool applied:
Tool 02: “Combined tool to identify the baseline scenario and demonstrate additionality(version07.0)”
Tool 08: “Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version03.0)”
Tool 14: “Project and leakage emissions from anaerobic digesters (Version 02.0)”
Tool 06:” Project emissions from flaring” (Version 4.0)
Tool 05:” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation” (Version 3.0)
Tool 24:” Common practice (Version 03.1)”

All above methodology and tool can be available from:
http://cdm.unfccc.int/methodologies/PAmethodologies/approved 
https://cdm.unfccc.int/Reference/tools/index.html
 
[bookmark: _Toc40962737]Crediting period of project 
>>
Start date of crediting period: 20/01/2021.
End date of crediting period:19/01/2026.
Total length of crediting period: 20/01/2021 to 19/01/2026 (first and last days included) for the first crediting period (two renewal cycles and in total 15 years). The 1st monitoring period is from 20/01/2021 to 31/03/2022 (first and last days included), which belong to the first crediting period.

Expected lifetime of the project: 15 years[footnoteRef:2]. [2:  As per purchase agreement of anaerobic tanks, the technical lifetime of anaerobic tanks is 20 years which is more than 15 years.] 



SECTION B. [bookmark: _Toc40962738][bookmark: _Ref47706306][bookmark: _Ref49860659]IMPLEMENTATION OF PROJECT 
[bookmark: _Toc40962739][bookmark: _Ref418094175]Description of implemented project 
>>
[bookmark: _Hlk77082346]9 sets of AWMSs in 9 swine farms have been implemented. All the manure and wastewater are collected and then be separated first. The separated solid is treated in aerobic composting system, which is used as fertilizer. And part of the fertilizer products is distributed to the surrounding farmers free of charge to improve the life condition of farmers, the others is sold to the market. The separated liquid is treated through anaerobic digestion, the biogas generated during the treatment process is captured for power generation. if there is surplus biogas, then the biogas can be flared through the flaring system. The sludge produced from anaerobic digestion is treated through aerobic composting together with the separated solid and the effluent is treated aerobically and then used for agriculture irrigation.

Anaerobic tanks adopt Upflow Anaerobic Sludge Bed Reactor (UASB) as its anaerobic digester technology, and the biogas generated from the anaerobic digesters enter the biogas generator set after biological desulfurization and dehydration purification. The generated electricity is used for daily operation of AWMSs and the swine farms, and the waste heat of the generator is recycled for increasing the temperature of the anaerobic reactor. At the same time, and the residual biogas is flared if there is any surplus biogas.

The technical flow of the project activity is shown below:
[bookmark: _Hlk72145106][image: ]
Figure 2 Process flow of biogas project in the swine farms

The project was implemented in 9 existing swine farms and the technology implemented at each swine farm was same. While the treatment capacities of each AWMS and the size of each swine farm and corresponding design of the AWMS was different. The treatment capacity and equipment of the system are designed according to the size of the farm. The construction date, commissioning date and start date of operation of AWMS in each farm are summarized in Table2. The other mainly milestone for implementation of the project are summarized in Table3. The volume for original uncovered anaerobic lagoons and the equipment parameters used of each swine farm are shown in the following Table 4:
Table 2 The construction, commissioning and start operation date of AWMS in each swine farm involved in this project
	Swine farm name
	Construction date
	Commissioning date
	Start Operation date

	Bama Yanyan swine farm
	15/09/2020
	13/01/2021
	20/01/2021

	Chongzuo Zuozhou swine Farm
	23/09/2020
	15/01/2021
	20/01/2021

	Tianyang Wucun swine Farm
	13/09/2020
	14/01/2021
	20/01/2021

	Quanzhou Dengjiabu swine Farm
	18/09/2020
	13/01/2021
	20/01/2021

	Chongzuo Quming swine Farm
	16/09/2020
	12/01/2021
	20/01/2021

	Jingxi swine Farm
	18/09/2020
	10/01/2021
	20/01/2021

	Liucheng Mashan swine Farm
	23/09/2020
	11/01/2021
	20/01/2021

	Tengxian Tianping swine Farm
	14/09/2020
	13/01/2021
	20/01/2021

	Debao Chengguan swine Farm
	16/09/2020
	14/01/2021
	20/01/2021



Table 3 Milestone for implementation of the project
	Time
	Main actions

	05/05/2020
	Project evaluation report

	07/07/2020
	EIA Approval by local Ecology and Environment Department

	05/09/2020
	Start date of the project, the date on signing biogas power generator purchase contract

	15/12/2020
	Training for the GS monitoring plan and biogas safety operation

	20/01/2021
	The project was put into operation

	01/09/2021
	Submission for preliminary review

	15/10/2021
	Local stakeholder consulting physical meeting

	13/12/2021
	Training for the GS monitoring plan and biogas safety operation



There are no deviations or delays compared to information in approved PDD. 

During this monitoring period, there was no special event occurred, such as overhaul and downtimes of anaerobic digesters. All the equipment operated well and no equipment was under maintenance during this monitoring period.

Table 4 technical parameters of main equipment and uncovered anaerobic lagoons

	[bookmark: _Hlk85733081]Farm name
	Bama Yanyan swine Farm
	Chongzuo Zuozhou swine Farm
	Tianyang Wucun swine Farm
	Quanzhou Dengjiabu swine Farm
	Chongzuo Quming swine Farm
	Jingxi swine Farm
	Liucheng Mashan swine Farm
	Tengxian Tianping swine Farm
	Debao Chengguan swine Farm

	Treatment capacities of AMMS(t/d)
	180
	100
	100
	50
	180
	200
	280
	150
	50

	Baseline anaerobic lagoon parameters

	Size of baseline anaerobic lagoon(length*width*depth) (m3)
	100*50*4
	50*50*4
	50*50*4
	50*40*3
	100*50*4
	100*50*4
	80*80*4
	100*50*3
	40*40*3

	technical life:
	No Less than 15 years

	Generator equipment parameters

	Type
	C650D5E
	C400D5E
	C350D5E
	C200D5E
	C800D5E
	C800D5E
	C1200D5E
	C600D5E
	C200D5E

	Rated power (kw)
	650
	400
	350
	200
	800
	800
	1200
	600
	200

	Rated current(A)
	450
	450
	450
	450
	450
	450
	450
	450
	450

	Rated speed (rpm)
	1500
	1500
	1500
	1500
	1500
	1500
	1500
	1500
	1500

	Equipment Quantity
	1
	1
	1
	1
	1
	1
	1
	1
	1

	Equipment technical life
	30 years

	Anaerobic tank parameters

	Design capacity (m3)
	3000
	2000
	2000
	1000
	3000
	3500
	4500
	2500
	1000

	Stay time(day)
	15.5-16
	15.5-16
	15.5-16
	15.5-16
	15.5-16
	15.5-16
	15.5-16
	15.5-16
	15.5-16

	Fermentation temperature(℃)
	35-38
	35-38
	35-38
	35-38
	35-38
	35-38
	35-38
	35-38
	35-38

	Equipment Quantity
	1
	1
	1
	1
	1
	2
	2
	1
	1

	Equipment technical life
	20 years

	Turnover machine parameters

	Type
	FP-2800
	FP-2800
	FP-2800
	FP-2800
	FP-2800
	FP-3800
	FP-3800
	FP-2800
	FP-2800

	Power(kw/H)
	4
	4
	4
	4
	4
	5.5
	5.5
	4
	4

	Speed of work(m/h)
	6.85
	6.85
	6.85
	6.85
	6.85
	6.85
	6.85
	6.85
	6.85

	Walking width(mm)
	2800
	2800
	2800
	2800
	2800
	3800
	3800
	2800
	2800

	Tossing speed (mm)
	50
	50
	50
	50
	50
	50
	50
	50
	50

	Equipment Quantity
	1
	1
	1
	1
	1
	1
	1
	1
	1

	Equipment technical life
	15 years

	Flared system

	Type
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare

	Material 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 
	304 stainless steels 

	Height (m)
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5

	Main wall thickness (mm)
	3
	3
	3
	3
	3
	3
	3
	3
	3

	Equipment technical life
	15 years







[bookmark: _Toc40962740]B.1.1 Forward Action Requests 
>>
As this monitoring period is the 1st monitoring period, so this part should describe the “Declare any Forward Action Requests from Design certification”. As the project developer of this project choose combine Design Certification with their first Verification and Performance Review, so there are no Forward Action Requests from Design certification to addressed.

Post-Design Certification changes
>>
[bookmark: _Ref418094308][bookmark: _Toc40962741]B.2.1. Temporary deviations from the approved Monitoring & Reporting Plan, methodology or standardized baseline
>>
NA
[bookmark: _Ref418094311][bookmark: _Toc40962742]B.2.2. Corrections
>>
NA
[bookmark: _Ref418094316][bookmark: _Toc40962743]B.2.3. Changes to start date of crediting period 
>>
NA
[bookmark: _Ref418094322][bookmark: _Toc40962744]B.2.4. Permanent changes from the Design Certified monitoring plan, applied methodology or applied standardized baseline
>>
NA
[bookmark: _Ref418094327][bookmark: _Toc40962745]B.2.5. Changes to project design of approved project
>>
NA



SECTION C. [bookmark: _Toc40962746][bookmark: _Ref47706319][bookmark: _Ref49860669]DESCRIPTION OF MONITORING SYSTEM APPLIED BY THE PROJECT
>>
Parameters to be monitored
According to section B.7.1 of the PDD, parameters need to be monitored is as following,

Table 5 monitoring parameter
	parameter
	Measurement methods and procedures

	For Mitigation Measure for Safeguarding Principles

	Employee Training of biogas safety operation
	Determined by the training Notice which was held once a year.
In this monitoring period, a total of two trainings were held. The first was conducted before the project was put into operation, all employees involved in this project was trained about and monitoring plan and biogas safety operation on 15/12/2020, the second training was conducted on 13/12/2021, which can be proved by training Notice and meeting attendance record.

	SDG 7

	Total electricity produced, EGd,y
	Measured continuously by the electric meters installed at the outlet of generator in each farm. Total 9 electric meters were installed. The electric meter reading was recorded daily by the staff and the electricity generation is not included during the commissioning period.
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity generation is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity generation.
The electricity meter was calibrated periodically by an officially accredited entity. Collected data is archived in both electronic and printed copies.  Detailed information on meters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	SDG 8

	Total number of jobs 
	Parameters for SDG 8 were determined based on Record keeping book and cross-checked by labor contract. 18 full-time jobs for local people were created in the 1st monitoring period (including 9 females and 9males).

	SDG 13

	[bookmark: _Hlk87272821]Number of animals of type LT produced annually for the year y, Np,LT
	[bookmark: _Hlk87272933]Each pig involved in this project has a unique electronic ear tag when was born, which is an electronic device dedicated to the identification and electronic management of animals, can track automatically. This electronic ear tag can be connected to the Data Collection System (DCS), which can store and read information. Therefore, the number of swine produced in the farm can be monitored through the auto tracking devices of electronic ear tag once pig slaughter monthly and obtained by the DCS.  At the same time, the technicians in farms record manually the number of swine produced in the farms monthly. So, this parameter can be sourced from “Export record form of Market swine”. Also, the monthly sale records for each farm can be crosschecked during this monitoring period.

	[bookmark: _Hlk87273021]Number of days animal of type LT is alive in the farm in the year y, Nda,LT
	The days of swine alive in the farm can be traced through the electronic ear tag by the technical staff in each farm and obtained by the DCS.  At the same time, the days of swine alive in the farm was recorded in the “Export record form of Market swine” manually by the responsible staff. Also, the monthly sale records for each farm used to crosschecked during this monitoring period.

	[bookmark: OLE_LINK1]Daily stock of animals in the farm, discounting dead and discarded animals, NAA,LT
	Each pig involved in this project has a unique electronic ear tag when was born, which is an electronic device dedicated to the identification and electronic management of animals, can track automatically. This electronic ear tag can be connected to the Data Collection System (DCS), which can store and read information. Therefore, this parameter can be monitored through the auto tracking devices of electronic ear tag. 
In this monitoring period, this parameter was recorded daily by the technicians in farms from the DCS system. The technicians in farms begin to record the daily stock number of animals from the first day of monitoring period, and this record data has included the new imported animal and discounting dead and discharge animals. The annual average number of animals (NAA,LT) was calculated based on the daily stock of breeding swine in the farms without considering dead animals and discarded animals. 

	Average animal weight of a defined livestock population at the project site, Wsite
	Measured by the weight measurers at the end of each month. One weight measure was equipped for each farm at least, total 9 weight measures were included for this project. Wsite was conducted by sampling in the three age groups (Nursery phase, Growing phase and Mature phase) of two type swine in each swine farm monthly. The weight data is recorded by the technicians in farms and then average animal weight of a defined livestock population at the project site was calculated based on these data. The weight measures were calibrated periodically by an officially accredited entity. Detailed calibration information on weight measures including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Number of days treatment plant was operational in year y, ndy
	Monitored and recorded by PP and the production record from the DCS system can be crosscheck that the treatment plant is operational.

	Fraction of volatile solids directed to aerobic treatment FAer
	According to the methodology, FAer should be monitored annually. However, there is no monitoring equip installed in the project activity to monitor the influent into anaerobic digestion and aerobic system during this monitoring period, therefore the value of FAer is applied as 100%, which is conservative and consistency with PDD.

	Biogas flow, Vf
	Measured by the biogas flow meters (biogas flow meter 1 installed at the outlet of the anaerobic digestion, biogas flow meter 2 installed at the inlet of the biogas generator and biogas flow meter 3 installed in the inlet of the flare system) continuously, record hourly and saved automatically in the Data Collection System (DCS). There were three flow meters in each farm and total 27 flow meters were included for this project. Daily biogas flow is equal to the cumulative value of 24 hours, and monthly biogas flow can be accumulated on daily basis.
The biogas flow meters used were calibrated periodically by an officially accredited entity. In addition, the biogas flow meter automatically measured the instantaneous flow rate, temperature and pressure per hour, so it is not necessary to install other equipment separately to measure the instantaneous flow rate (Vt,db), the biogas temperature (Tt) and pressure (Pt). Collected data is archived in both electronic and printed copies. Detailed information on flowmeters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Quantity of electricity consumed by the proposed project in year y, ECPJ,j,y
	Measured continuously by the electric meters installed in project site in each farm. Total 9 electric meters were installed in this project. The electric meter reading was recorded daily and summarized monthly by the staff and the electricity consumption is not included during commissioning period.
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity consumption is equal to the difference between the previous day's and the next day's readings. 
The staff in each swine farm recorded the meter reading at 24:00 of last day in each month and then reported the monthly electricity consumption to the grid company. The grid company checked and supplied the grid statement of the meters to the PP monthly.
The electricity meter was calibrated periodically by an officially accredited entity. Collected data is archived in both electronic and printed copies. Detailed information on meters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Average technical transmission and distribution losses for providing electricity to source j in year y, TDLj,y
	Sourced from Tool 05” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation (version 03.0)”, the value is 20% in this monitoring period. This value will be renewed once the tool is updated.

	Volumetric flow of the gaseous stream in time interval t on a dry basis, Vt,db
	Measured by flowmeters, which can record hourly and saved automatically in the DCS system. As per described in monitoring parameter Vf, the flowmeters to monitor Vt,db are the same as the flowmeters that monitor Vf since the flowmeter can monitor other parameter such as Vt,db, Tt and Pt simultaneously. So, the data can be obtained from the system and the monthly data was exported by the staff at the beginning of next month. Daily biogas flow is equal to the cumulative value of 24 hours, and monthly biogas flow can be accumulated on daily basis. Original collected data can be exported through the system and is archived in electronic.

	Volumetric fraction of greenhouse gas i in a time interval t on a dry basis, m³ gas i/m³ dry gas, Vi,t,db
	Continuously measurement and record hourly by online gas analyser installed at the outlet of the anaerobic digester and saved automatically in the DCS system. One gas analyser was equipped in each farm and there are 9 gas analysers totally. Therefore, the data can be obtained from system and the monthly data was exported by the staff at the beginning of next month. Daily and monthly CH4 concentration was calculated based on the 24-hour average and daily average CH4 concentration. 
Gas analyzers were calibrated periodically by an officially accredited entity. Original collected data can be exported through the system and is archived in electronic. Detailed information on gas analyzers including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Temperature of the gaseous stream in time interval t, Tt;
Pressure of the gaseous stream in time interval t, Pt.
	Continuously Measurement by the biogas flow meter, which can record hourly and saved automatically in the DCS system. As per described in monitoring parameter Vf, the flowmeters to monitor Tt and Pt are the same as the flowmeters that monitor Vf since the flowmeter can monitor other parameter such as Vt,db, Tt and Pt simultaneously. So, the data can be obtained from DCS system and the monthly data was exported by the staff at the beginning of next month. Daily and monthly Temperature and Pressure of the biogas flow was calculated based on the 24-hour average and daily average values. Original collected data can be exported through the system and is archived in electronic. 
Detailed information on Flow meters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Density of greenhouse gas i in the gaseous stream in time interval t, ρi,t
	[bookmark: OLE_LINK3]This parameter was calculated based on the temperature and pressure of the gaseous stream in time interval t. The monitor of the temperature and pressure of the gaseous stream see the description of the above two parameters in this table.

	Fraction of manure handled in system j in project activity MS%j, MS%j
	As there is no equipment installed to monitor this parameter in the actual operation. so, in the monitoring period, to be conservative, the value of this parameter in the emission reduction calculation is 100%.

	Maximum methane producing potential of the volatile solid generated by animal type LT, B0, LT
	Not monitored during this monitoring period and the value is taken from IPCC 2006, which is a published source. The parameter value will be updated on latest available public data source.

	Type of barn and AWMS, Type
	During this monitoring period, the type of barn and AWMS was not changed as the design. 

	Annual average ambient temperature at project site， T
	[bookmark: _Hlk104544931][bookmark: _Toc376879902][bookmark: _Toc376882518][bookmark: _Toc377134813][bookmark: _Toc376881433][bookmark: _Toc376879108]The average  project site temperature in 2021 is 21.6[footnoteRef:3]℃, which is a Publicly available data.  [3:  https://k.sina.cn/article_7517400647_1c0126e4705902b4do.html] 

In this monitoring period, the average  project site temperature in 2021 is 21.6℃. In addition, as this monitoring period only includes the first 3 months of 2022 year and the temperature in first 3 months cannot represent the whole 2022 year, also the annual average temperature in 2022 is not yet available, So, in this monitoring period, the Annual average ambient temperature at project site of 2022 applied the value of 2021.
After comparing the actual temperature (21.6℃) and the temperature of ex-ante estimated(17.5~23.5℃), So, in this monitoring period, MCFj value is 76% with the lower temperature of 17.5°C as per Appendix 3 of ACM0010(Version 08.0). Then multiplying MCF values with a value of 0.94, so 71.44% of MCFj is used for calculation during in this monitoring period.

	Annual average nitrogen excretion per head of a defined livestock population estimated as described in Appendix 2, NEXLT
	Not monitored during this MR since the parameter is calculated as the equation of option 2 in Appendix 2 of methodology ACM0010 Version 08.0 and the value of other parameter applied in the equation is taken from IPCC 2006, which is a published source. The parameter value will be updated on latest available public data source.




Monitoring framework
[bookmark: _Hlk56590379][bookmark: _Hlk87279254]The project owner is responsible for the whole monitoring work. The GS Monitoring Team is established to collect and record monitoring data within the project boundary. The GS monitoring team is responsible for the normal operation of the AWMSs and the collection and record of all the monitoring data. All the data is reviewed by the project developer and VVB. Each member of the GS monitoring team is trained by the project owner at least once a year. The overall monitoring system structure of the project shows as below:


Figure 3 The Organization Structure of the Monitoring Team

Monitoring equipment and installation
Installation and configuration of monitoring equipment are shown as Figure 4.  In order to ensure measurements with a low degree of uncertainty, the data monitoring equipment have been calibrated and checked by appropriately qualified third party according to appropriate national standard. 

For this monitoring period, all the monitoring equipment were calibrated according to relevant regulations.
[image: ]
[bookmark: _Hlk81557214]Figure 4 The monitoring system of the project (Same monitoring system for each farm)

Corrective actions
The whole GS monitoring team fellow recognized standard data evaluation methods to guarantee that the data was reliable and accurate. There was no correction of nonconformities occurred in implementation of the project or the monitoring plan during the 1st monitoring period. For QA/QC procedure, please refer to QA/QC procedures in section D.2 of the monitoring report.

Data management
Records are the most important exercise in relation to the monitoring process. Without accurate and efficient record keeping, project emission reductions cannot be verified. 

Once missing data on a given day or a certain period of time happened, the most appropriate values such as daily average or monthly average will be used for calculation, which is to ensure that emission reductions are conservative.

All data collected as part of the monitoring plan shall be archived in electronic form and paper until at least two years after the entry period. 

[bookmark: _Hlk88143535]Emergency procedure
Employees need to be familiar with the process flow and emergency situations that may occur during project operation and operate in strict accordance with the technical specifications of each process treatment equipment and monitoring equipment. During the operation of the project, all equipment and related instruments shall be checked regularly according to the manufacturer’s recommendations. If necessary, calibration and/or proper repair have to be carried out immediately.

In case of malfunction and/or damage of any system or piece of the process, it may cause damage to the operation of the system, especially serious damage to the biogas generation system and combustion system it must be dealt with as soon as possible and reported to the responsible technician immediately.

There was no emergency happened during this monitoring period.

Avoiding of double counting
All swine farms involved in this project can be identified through its GPS coordinates, which will prevent the farms counted in the project activity to be part of any other voluntary market or emission reduction mechanism (CDM, CCER, VCS etc.) as well. Besides, the project owner has signed the Declaration of No Double Counting Statement and Declaration of not involved in other GHG scheme on 30/05/2021. The emission reductions were not double counted during the 1st monitoring period.

Table 6 General description of monitoring equipment
	[bookmark: _Hlk80952523]Monitoring equipment
	Parameter to be monitored
	Installed location
	Type
	Series number
	Accuracy
	Date of calibration
	Calibration standard
	Validity
	Calibration agency

	Flow meter 1
	Vf
Tt
 Pt
	at the outlet of the anaerobic digestion
	HD-LUB
	Please refer to below Table 7
	1.5
	08/01/2021
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter)
	07/01/2023
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Flow meter 2
	Vf
Tt
 Pt
	at the inlet of generator
	HD-LUB
	
	1.5
	08/01/2021
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter)
	07/01/2023
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Flow meter 3
	Vf
Tt
 Pt

	in inlet of flare
	HD-LUB
	
	1.5
	08/01/2021
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter)
	07/01/2023
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Electricity meter 1
	EGd,y
	in the project site
	DSSD331
	
	0.5s
	11/01/2021
	JJG596-2012 (Electrical Meters for Measuring Alternating-current Electrical Energy)
	10/01/2026
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Electricity meter 2
	ECPJ,j,y
	at the outlet of generator
	DSSD331
	
	0.5s
	11/01/2021
	JJG596-2012 (Electrical Meters for Measuring Alternating-current Electrical Energy)
	10/01/2026
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Weight measurer
	wsite
	in each pig farm
	XK3190-A12+(E)
	
	Ⅲ level
	12/12/2020, 10/12/2021
	JJG539-2016(Digital Indicator Scale Verification Regulations)
	11/12/2021, 09/12/2022
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing

	Gas analyzer
	Vi,t,db
	at the outlet of the anaerobic digesters
	   Gasboard-9060  
	
	1%
	08/01/2021,
06/01/2022
	[bookmark: OLE_LINK5]JJG693-2011(Verification Regulation of Alarmer Detectors of Combustible Gas)
	07/01/2022,
05/01/2023
	Guangxi Zhuang Autonomous Region Institute of Metrology and testing



Table 7 Series number of monitoring equipment
	Swine farm
	Series number

	
	Flowmeter 1
	Flowmeter 2
	Flowmeter 3
	Electricity meter 1
	Electricity meter 2
	Weight measurer
	Gas analyzer

	Bama Yanyan swine farm
	202001002357
	202001002358
	202001002359
	120236
	120237
	2018465447
	2021010637

	Chongzuo Zuozhou swine Farm
	202002003518
	202002003519
	202002003520
	180877
	180878
	2018375816
	2021010315

	Tianyang Wucun swine Farm
	202001006849
	202001006850
	202001006851
	146742
	146743
	2019139409
	2021010409

	Quanzhou Dengjiabu swine Farm
	202003001748
	202003001749
	202003001750
	158112
	158113
	2018470848
	2020122503

	Chongzuo Quming swine Farm
	202002005473
	202002005474
	202002005475
	162261
	162262
	2018581267
	2021010621

	Jingxi swine Farm
	202003002189
	202003002190
	202003002191
	180946
	180947
	2018252942
	2020122809

	Liucheng Mashan swine Farm
	202002002847
	202002002848
	202002002849
	218445
	218446
	2019452136
	2020010719

	Tengxian Tianping swine Farm
	202001004638
	202001004639
	202001004640
	178004
	178005
	2018379283
	2020010247

	Debao Chengguan swine Farm
	202003000432
	202003000433
	202003000434
	207758
	207759
	2018581048
	2021010503




SECTION D. [bookmark: _Toc40962747][bookmark: _Ref47706326][bookmark: _Ref49860677]DATA AND PARAMETERS
[bookmark: _Ref418094907][bookmark: _Toc40962748]Data and parameters fixed ex ante or at renewal of crediting period
>>
SDG13
	Data/parameter
	GWPCH4

	Unit
	tCO2e/tCH4

	Description
	Global Warming Potential of CH4

	Source of data
	IPCC Fifth Assessment Report

	Value(s) applied
	28

	Choice of data or Measurement methods and procedures 
	100-year values are adopted from IPCC Fifth Assessment Report

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	All monitoring, verifications and requests for performance certification of Certified products and / or Impact Statements for the period starting 01 January 2021 shall use the AR5 GWP values (28) for calculating emission reductions and removals according to applicability of global warming potential for gold standard for the global goals projects.




	Data/parameter
	GWPN2O

	Unit
	tCO2e/tN2O

	Description
	Global Warming Potential of N2O

	Source of data
	IPCC Fifth Assessment Report

	Value(s) applied
	265

	Choice of data or Measurement methods and procedures 
	100-year values are adopted from IPCC Fifth Assessment Report

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	All monitoring, verifications and requests for performance certification of Certified products and / or Impact Statements for the period starting 01 January 2021 shall use the AR5 GWP values (265) for calculating emission reductions and removals according to applicability of global warming potential for gold standard for the global goals projects.



	Data/parameter
	DCH4

	Unit
	t/m3

	Description
	Density of CH4 

	Source of data
	ACM0010 Version 08.0

	Value(s) applied
	0.00067

	Choice of data or Measurement methods and procedures 
	0.00067 t/m3 at room temperature 20℃ and 1 atm pressure.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	N/A




	Data/parameter
	MCFj

	Unit
	-

	Description
	Methane conversion factor for the baseline AWMSj

	Source of data
	IPCC 2006 Table 10.17, chapter 10, volume 4 

	Value(s) applied
	71.44%

	Choice of data or Measurement methods and procedures 
	MCFj value for uncovered anaerobic lagoon (baseline AWMS) is chosen.
	
A conservativeness factor has been applied by multiplying MCFj value (i.e., 76%) with a value of 0.94, to account for the 20 per cent uncertainty in the MCFj values as reported by IPCC 2006. 
For this project, the actual annual average temperature in 2021 is 21.6°C and the average temperature used for pre calculation is 17.5~23.5°C. In addition, as this monitoring period only includes the first 3 months of 2022 year and the temperature in first 3 months cannot represent the whole 2022 year, also the annual average temperature in 2022 is not yet available, So, in this monitoring period, the MCFj value of 2022 applied the value of 2021. After comparing to the actual annual average temperature and average temperature used for pre calculation, the MCFj value is 76% with the lower temperature of 17.5°C as per Appendix 3 of ACM0010(Version 08.0). Then multiplying MCF values with a value of 0.94, so 71.44% of MCFj is used for calculation during in this monitoring period. 

	Purpose of data
	project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	MS%Bl,j

	Unit
	Fraction

	Description
	Fraction of manure handled in system j in the baseline. 

	Source of data
	Project proponents 

	Value(s) applied
	100%

	Choice of data or Measurement methods and procedures 
	In this project, the baseline manure management system is uncovered anaerobic lagoon only. The amount of manure handled by the anaerobic lagoon is 100%. 

	Purpose of data
	Calculation of baseline emissions

	Additional comment
	N/A



	Data/parameter
	Wdefault

	Unit
	kg

	Description
	[bookmark: OLE_LINK52]Default average animal weight of a defined population

	Source of data
	IPCC 2006 Table 10A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	Wdefault (Market swine) =28kg
Wdefault (Breeding swine) =28kg

	Choice of data or Measurement methods and procedures 
	The values in IPCC 2006 and US-EPA are compared and the lower value from IPCC 2006 is applied.

	Purpose of data
	Calculation of Baseline emissions

	Additional comment
	N/A



	Data/parameter
	VSdefault

	Unit
	kg-dm/animal/day

	Description
	Default value for the volatile solid excretion per day on a dry-matter basis for a defined livestock population

	Source of data
	IPCC 2006 Table 10A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	VSdefault(Market swine)=0.3
VSdefault(Breeding swine)=0.3

	Choice of data or Measurement methods and procedures 
	The values in IPCC 2006 and US-EPA are compared and the lower value from IPCC 2006 is applied.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	N/A




	Data/parameter
	Nrate(T)

	Unit
	kg N (1000 kg animal mass)-1 day-1 

	Description
	default N excretion rate

	Source of data
	IPCC 2006 Table 10.19, chapter 10, volume 4

	Value(s) applied
	Nrate(T) (Market swine) =0.42
Nrate(T)(Breeding swine) =0.24

	Choice of data or Measurement methods and procedures 
	Default value from IPCC 2006 is applied.

	Purpose of data
	NEXIPCC default calculations

	Additional comment
	N/A



		Data/parameter
	NEXIPCC default

	Unit
	kg N/ animal/year 

	Description
	Default value for the nitrogen excretion per head of a defined livestock population

	Source of data
	Calculated by the equation: 
NEXIPCC default =Nrate(T)* TAM/1000*365[footnoteRef:4] [4:  365 in this formula represents 365 days per year, which corresponds to the unit of this parameter: kg N / animal / year and Nrate(T) means the default N excretion rate with the unit of kg N/ (1000 kg animal mass)/ day However, this monitoring period is 20/01/2021-31/03/2022, more than one year. Therefore, this parameter should be calculated according to the actual number of days.] 


	Value(s) applied
		Period
	Market Swine
	Breeding Swine

	20/01/2021-31/01/2021
	0.14
	0.08

	01/02/2021-28/02/2021
	0.33
	0.19

	01/03/2021-31/03/2021
	0.36
	0.21

	01/04/2021-30/04/2021
	0.35
	0.20

	01/05/2021-31/05/2021
	0.36
	0.21

	01/06/2021-30/06/2021
	0.35
	0.20

	01/07/2021-31/07/2021
	0.36
	0.21

	01/08/2021-31/08/2021
	0.36
	0.21

	01/09/2021-30/09/2021
	0.35
	0.20

	01/10/2021-31/10/2021
	0.36
	0.21

	01/11/2021-30/11/2021
	0.35
	0.20

	01/12/2021-31/12/2021
	0.36
	0.21

	01/01/2022-31/01/2022
	0.36
	0.21

	01/02/2022-28/02/2022
	0.33
	0.19

	01/03/2022-31/03/2022
	0.36
	0.21




	Choice of data or Measurement methods and procedures 
	NEXIPCC default is calculated as equation 10.30 in IPCC2006, Nrate(T) and TAM are default value from IPCC 2006.

	Purpose of data
	Baseline, Project and leakage emissions calculations

	Additional comment
	N/A



	Data/parameter
	TAM

	Unit
	kg animal-1 

	Description
	typical animal mass for livestock category

	Source of data
	IPCC 2006 Table 40A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	TAM (Market swine) =28
TAM (Breeding swine) =28

	Choice of data or Measurement methods and procedures 
	Default value from IPCC 2006 is applied.

	Purpose of data
	NEXIPCC default calculations

	Additional comment
	N/A




	Data/parameter
	Fgas MS,j,LT

	Unit
	Fraction

	Description
	Default values for nitrogen loss due to volatilization of NH3 and NOX from manure management

	Source of data
	IPCC 2006 Table 10.22, chapter 10, volume 4

	Value(s) applied
	FgasMS,j,LT,  (anaerobic lagoon) : 40%
FgasMS,j,LT ,  (solid storage) : 45%

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	EFN2O,D,j

	Unit
	Kg N2O-N/kg N

	Description
	Direct N2O emission factor for the treatment system j of the manure management system

	Source of data
	IPCC 2006 Table 10.21, chapter 10, volume 4

	Value(s) applied
	EFN2O,D,j=0 for anaerobic lagoon and digester, EFN2O,D,j =0.01 for aerobic lagoon 

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	[bookmark: OLE_LINK54]Data/parameter
	EFN2O,ID

	Unit
	kgN2O-N/kg NH3-N and NOX-N

	Description
	Indirect N2O emission factor for the treatment system j of the manure management system

	Source of data
	IPCC 2006 Table 11.3, chapter 11, volume 4

	Value(s) applied
	0.01 

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	EFCH4,default

	Unit
	t CH4 leaked / t CH4 produced

	Description
	Default emission factor for the fraction of CH4 produced that leak from the anaerobic digester (fraction)

	Source of data
	Tool 14:” Project and leakage emissions from anaerobic digesters (version 02.0)

	Value(s) applied
	0.05

	Choice of data or Measurement methods and procedures 
	UASB (Upflow Anaerobic Sludge Blanket) type digesters, floating gas holders with no external water seal

	Purpose of data
	Calculation of project emissions

	Additional comment
	PECH4,y for ex ante estimation adopted equation(4) of  Methodological tool “Project and leakage emissions from anaerobic digesters”, the amount of biogas collected at the digester will be monitored in section B.7 of PDD.




	Data/parameter
	RVS,n

	Unit
	Fraction

	Description
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated

	Source of data
	Refer to Appendix 1 of methodology ACM0010 

	Value(s) applied
	RVS,n, aerobic treatment and anaerobic digester: 20%, 80% for  leakage N2O emission released during project activity
RVS,n, one cell lagoon :85% for leakage N2O emission released during baseline scenario

	Choice of data or Measurement methods and procedures 
	Estimated from Table provided in Appendix 1 of ACM0010. The most conservative value for the given technology must be used.

	Purpose of data
	project emission/ leakage calculation

	Additional comment
	N/A



	Data/parameter
	RN,n

	Unit
	Fraction

	Description
	Nitrogen reduction factor 

	Source of data
	Refer to Appendix 1 of methodology ACM0010

	Value(s) applied
	RN,n, project activity(aerobic treatment and anaerobic digester): 5%,25%
RN,n, baseline ( uncovered anaerobic lagoon) : 80%

	Choice of data or Measurement methods and procedures 
	Anaerobic digester has been assumed as a covered first cell of two cell lagoon.
Uncovered anaerobic lagoon has been assumed as one cell lagoon.
The most conservative value for the given technology has been used.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A




	Data/parameter
	EF1, EF4, EF5

	Unit
	kg N2O-N/kg N for EF1, EF5 and [kg N2O-N/(kg NH3-N and NOX-N) for EF4

	Description
	Emission factor for N2O emissions from N inputs; from N leaching and runoff; from atmospheric deposition of N on soils and water surfaces 

	Source of data
	IPCC 2006 Guidelines default values are be used, since country specific or region-specific data are not available. EF1 from Table 41.1, chapter 11, volume 4. EF4 and EF5 from Table 41.3, chapter 11, volume 4

	Value(s) applied
	EF1 = 0.010
EF4 =0.010
EF5 = 0.0075

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	Fgasm

	Unit
	Fraction

	Description
	Fraction of N lost due to volatilization

	Source of data
	Default values from Table 11.3, chapter 11, volume 4 of IPCC 2006 guidelines 

	Value(s) applied
	0.2

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	Fleach

	Unit
	Fraction

	Description
	Fraction of all N added to/mineralized in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff

	Source of data
	Default values from Table 11.3, chapter 11, volume 4 of IPCC 2006 guidelines 

	Value(s) applied
	0.3

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	MCFd

	Unit
	-

	Description
	Methane conversion factor for leakage calculation

	Source of data
	Methodology ACM0010(version 08.0)

	Value(s) applied
	1

	Choice of data or Measurement methods and procedures 
	According to paragraph 51 of the methodology ACM0010” GHG emission reductions from manure management systems (version 08.0)”, Methane conversion factor for leakage calculation assumed to be equal 1

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	EFEF,j,y

	Unit
	tCO2/MWh

	Description
	Emission factor for electricity generation 

	Source of data
	Published by Ministry of Ecology and Environment of the People's Republic of China, which is the DNA of China

	Value(s) applied
	0.50885

	Choice of data or Measurement methods and procedures 
	According to tool” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”

	Purpose of data
	Calculation of project emission

	Additional comment
	N/A



	Data/parameter
	Ru

	Unit
	Pa.m3/kmol.K 

	Description
	Universal ideal gases constant 

	Source of data
	Tool 08:” Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version 03.0)”

	Value(s) applied
	8,314

	Choice of data or Measurement methods and procedures 
	Value is fixed as Tool 08

	Purpose of data
	Calculation of project emission

	Additional comment
	/



	Data/parameter
	MMi

	Unit
	kg/kmol 

	Description
	Molecular mass of greenhouse gas I  

	Source of data
	Tool 08:” Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version 03.0)”

	Value(s) applied
	16.04 kg/mol for methane

	Choice of data or Measurement methods and procedures 
	Value is fixed as Tool 08

	Purpose of data
	Calculation of project emission

	Additional comment
	/




	Data/parameter
	ηflare,m

	Unit
	%

	Description
	Flare efficiency in minute m

	Source of data
	Tool 06” Project emissions from flaring (Version 04.0)”

	Value(s) applied
	0%

	Choice of data or Measurement methods and procedures 
	0% is the conservative value.

	Purpose of data
	Calculation of project emission

	Additional comment
	/



[bookmark: _Ref418094911][bookmark: _Toc40962777]Data and parameters monitored
>>
SDG 13
	Data / Parameter
	Np,LT

	Unit
	Number

	Description
	Number of animals of type LT produced annually for the year y 

	Source of data
	Production record of market swine

	Value(s) of monitored parameter
		Period
	Np,LT

	20/01/2021-31/01/2021
	9,820 heads of market swine

	01/02/2021-28/02/2021
	26,062 heads of market swine

	01/03/2021-31/03/2021
	25,923 heads of market swine

	01/04/2021-30/04/2021
	25,690 heads of market swine

	01/05/2021-31/05/2021
	25,880 heads of market swine

	01/06/2021-30/06/2021
	25,949 heads of market swine

	01/07/2021-31/07/2021
	25,825 heads of market swine

	01/08/2021-31/08/2021
	25,926 heads of market swine

	01/09/2021-30/09/2021
	25,621 heads of market swine

	01/10/2021-31/10/2021
	25,817 heads of market swine

	01/11/2021-30/11/2021
	25,851 heads of market swine

	01/12/2021-31/12/2021
	25,759 heads of market swine

	01/01/2022-31/01/2022
	25,840 heads of market swine

	01/02/2022-28/02/2022
	25,780 heads of market swine

	01/03/2022-31/03/2022
	25,624 heads of market swine

	Total
	371,367 heads of market swine




	Measurement methods and procedures
	To be collected for each swine population in all of the pig barns.  The number of swine produced in the swine farms had been recorded in the “Export record form of Market swine” manually by the responsible staff. 
Please refer to Section C of the MR for more details.

	Monitoring frequency
	Monitored monthly.

	QA/QC procedures
	Archive electronically during project plus 5 years.

	Purpose of data
	Use for the calculation of NLT

	Additional comment
	According to the Equation 4 in this MR, the calculated NLT is 152,828 heads (371,367heads*180days/365days/14.38months*12months)[footnoteRef:5]. However, according to the number of market pigs produced annually of each farm, the NLT calculated by Equation 4 is rounded to an integer as 152,825 heads. According to the conservative principle, the 152,825 heads was applied in the calculations of emission reductions in MR. [5:  For the monitoring period 20/01/2021-31/03/2022, it is about 14.38 months. therefore, the annual swine produced can be averaged according to the total quantity of swine produced during this monitoring period.] 

Np,LT has been cross-checked through the monthly sale records of 9 swine farms during this monitoring period. And the values between the Export record form of Market swine and the monthly sale records are consistent.
Therefore, Np,LT is reasonable and credible. 



	Data / Parameter
	Nda,LT

	Unit
	Number

	Description
	Number of days animal of type LT is alive in the farm in the year y

	Source of data
	Production record of market swine

	Value(s) of monitored parameter
		Period
	Nda,LT
	Period
	Nda,LT

	20/01/2021-31/01/2021
	180days
	01/09/2021-30/09/2021
	180days

	01/02/2021-28/02/2021
	180days
	01/10/2021-31/10/2021
	180days

	01/03/2021-31/03/2021
	180days
	01/11/2021-30/11/2021
	180days

	01/04/2021-30/04/2021
	180days
	01/12/2021-31/12/2021
	180days

	01/05/2021-31/05/2021
	180days
	01/01/2022-31/01/2022
	180days

	01/06/2021-30/06/2021
	180days
	01/02/2022-28/02/2022
	180days

	01/07/2021-31/07/2021
	180days
	01/03/2022-31/03/2022
	180days

	01/08/2021-31/08/2021
	180days
	
	




	Measurement methods and procedures
	The days of swine alive in the farm was recorded in the “Export record form of Market swine” manually by the responsible staff.  

	Monitoring frequency
	Monitored monthly.

	QA/QC procedures
	Archive electronically during project plus 5 years.

	Purpose of data
	Use for the calculation of NLT

	Additional comment
	The number of days the animal alive in the farm sourced from the “Export record form of Market swine” and was crosschecked through the “monthly sale records” of 9 swine farms during this monitoring period and it can be concluded that the data is consistent.
In addition, this value is in line with the number of days for pigs to be slaughtered by existing large-scale breeding groups in China[footnoteRef:6]. [6:  https://zhuanlan.zhihu.com/p/38676811
http://finance.people.com.cn/n1/2017/1121/c1004-29658996.html] 




	Data / Parameter
	NAA,LT

	Unit
	Number

	Description
	Daily stock of animals in the farm, discounting dead and discarded animals

	Source of data
	[bookmark: _Hlk100749885]Daily stock record of breeding swine  

	Value(s) of monitored parameter
		Period
	NAA,LT

	20/01/2021-31/01/2021
	89,885 heads of breeding swine

	01/02/2021-28/02/2021
	89,832 heads of breeding swine

	01/03/2021-31/03/2021
	89,845 heads of breeding swine

	01/04/2021-30/04/2021
	89,915 heads of breeding swine

	01/05/2021-31/05/2021
	89,809 heads of breeding swine

	01/06/2021-30/06/2021
	89,754 heads of breeding swine

	01/07/2021-31/07/2021
	89,905 heads of breeding swine

	01/08/2021-31/08/2021
	89,670 heads of breeding swine

	01/09/2021-30/09/2021
	89,854 heads of breeding swine

	01/10/2021-31/10/2021
	89,790 heads of breeding swine

	01/11/2021-30/11/2021
	89,905 heads of breeding swine

	01/12/2021-31/12/2021
	89,761 heads of breeding swine

	01/01/2022-31/01/2022
	89,894 heads of breeding swine

	01/02/2022-28/02/2022
	89,820 heads of breeding swine

	01/03/2022-31/03/2022
	89,703 heads of breeding swine

	Average
	89,823 heads of breeding swine




	Measurement methods and procedures
	Monitored daily through the auto tracking devices of electronic ear tag and the data can be obtained from DCS. The technicians in farms record the daily stock number of animal in “Breeding Swine stock record”, and this record data including the new imported animal and discounting dead and discharge animals. Archive electronically during project plus 5 years 
Please see the Section C of MR for details.

	Monitoring frequency
	daily

	QA/QC procedures
	The system on monitoring the number of livestock population was described in the PDD.

	Purpose of data
	Use for the calculation of baseline/project emission and leakage

	Additional comment
	The system on monitoring the daily stock of breeding swine in the farm was descried in Section C of MR. 



	Data / Parameter
	Wsite

	Unit
	kg

	Description
	Average animal weight of a defined livestock population at the project site

	Source of data
	Weight record table

	Value(s) of monitored parameter
		Period
	Market swine
	Breeding swine

	20/01/2021-31/01/2021
	60.8
	79.6

	01/02/2021-28/02/2021
	61.6
	77.1

	01/03/2021-31/03/2021
	62.2
	77.5

	01/04/2021-30/04/2021
	62.2
	78.0

	01/05/2021-31/05/2021
	61.3
	78.5

	01/06/2021-30/06/2021
	61.3
	77.8

	01/07/2021-31/07/2021
	61.3
	77.9

	01/08/2021-31/08/2021
	62.1
	78.1

	01/09/2021-30/09/2021
	61.6
	77.5

	01/10/2021-31/10/2021
	61.4
	77.4

	01/11/2021-30/11/2021
	60.6
	77.5

	01/12/2021-31/12/2021
	61.7
	77.5

	01/01/2022-31/01/2022
	60.4
	79.4

	01/02/2022-28/02/2022
	61.6
	77.9

	01/03/2022-31/03/2022
	62.0
	77.9

	Average
	61.5
	78.0




	Measurement methods and procedures
	[bookmark: OLE_LINK2]Measured by the weight measurers and record by the technical staff in each farm monthly
Please refer to Section D.4 of the MR for more details.

	Monitoring frequency
	monthly

	QA/QC procedures
	As this project involved 9 swine farms and two types of swine i.e., Market swine and Breeding swine, and as per applied methodology, each defined livestock population should be classified into a minimum of three age categories (The three age categories of marketing swine are classified according to the age in days, i.e., Nursery phase with 30-60days, Growing phase with 60-130days and Mature phase with 130-180days. The three age categories of breeding swine are classified according to the age in days, i.e., Nursery phase with 30-70days, Growing phase with 70-220days and Mature phase with 220-310days.), so the sampling method is Stratified random sampling. The specific sampling methods are as follows:
The sampling method is followed as PDD and described as below during this monitoring period.
1. the overall sample size based on the design population of pigs in each farm firstly is calculated as described in PDD. 
2. As the project involved 9 swine farms, then the sample size in each swine farm is determined based on the proportion of the number of each farm in the total number of 9 farms. 
3. Similarly, the sample size of each age group of Market swine and Breeding swine in each farm is also calculated based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in the farm.   
4. After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample is conducted in every swine farm. Since swine in different age are kept in the different pig houses, samples can be randomly selected from pig houses of this age group. 
5. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. 
6. [bookmark: _Hlk95292304]The sample will be marked after weighting and if the sample swine is still drawn next month, then this sample swine needs to be discarded and a new sample swine is drawn. This will be done every month until the end of the monitoring period.

	Purpose of data
	Used for estimating VSLT,y

	Additional comment
	Please see section D.4 for detail about sampling.



	Data/parameter
	ndy

	Unit
	number

	Description
	Number of days treatment plant was operational in year y.

	Source of data
	Project proponents

	Value(s) of monitored parameter
	The actual number of days 9 treatment plants that was operational are 436 days during this monitoring periods 
	Period
	ndy
	Period
	ndy

	20/01/2021-31/01/2021
	12
	01/09/2021-30/09/2021
	30

	01/02/2021-28/02/2021
	28
	01/10/2021-31/10/2021
	31

	01/03/2021-31/03/2021
	31
	01/11/2021-30/11/2021
	30

	01/04/2021-30/04/2021
	30
	01/12/2021-31/12/2021
	31

	01/05/2021-31/05/2021
	31
	01/01/2022-31/01/2022
	31

	01/06/2021-30/06/2021
	30
	01/02/2022-28/02/2022
	28

	01/07/2021-31/07/2021
	31
	01/03/2022-31/03/2022
	31

	01/08/2021-31/08/2021
	31
	Total
	436




	Measurement methods and procedures
	The staff in each manure treatment plant record the number of operation days daily and then record the total monthly number of operation days in end of each month through monthly operation record.

	Monitoring frequency
	Daily

	QA/QC procedures
	The accumulated meter reading of flowmeters installed in the outlet of anaerobic digesters in each farm daily can be demonstrated that the AWMSs are actually running on a daily basis. The 9 treatment plants is operational every day during this monitoring period according to the actual daily reading of flowmeters installed in the outlet of anaerobic digesters in each farm.

	Purpose of data
	Calculation of Baseline emissions

	Additional comment
	ndy is the number of days treatment plants was operational. As the anaerobic fermentation is the main process of the treatment process for the project, so the operating days of the anaerobic tank in each farm can be considered as the operating days of the treatment plant. as long as the anaerobic tank is running, biogas will be generated, so the period of biogas generation monitored by the flow meter is the operating days of the treatment plant. Therefore, each farm was operational for 436 days and there was no breakdown/ non –operational day at any of the farms according to the daily meter reading of flowmeter installed in the outlet of anaerobic digesters in each farm.



	Data / Parameter
	FAer

	Unit
	Fraction

	Description
	Fraction of volatile solids directed to aerobic treatment

	Source of data
	PDD

	Value(s) of monitored parameter
	100%

	Measurement methods and procedures
	As this parameter is not monitored in the actual operation. So, in the monitoring period, to be conservative, the value of this parameter in the emission reduction calculation is 100%, which is consistent with PDD.

	Monitoring frequency
	Annually 

	QA/QC procedures
	Value of FAer is applied as 100%, which is conservative.

	Purpose of data
	Calculation of project emission

	Additional comment
	N/A



	[bookmark: _Hlk77239910]Data/parameter
	vf

	Unit
	m3

	Description
	Biogas flow 

	Source of data
	Project proponents

	Value(s) of monitored parameter
		period
	Vf1-   outlet of the anaerobic digestion (m3)
	Vf2- inlet of biogas generator (m3)
	Vf3- inlet of flare system (m3)

	20/01/2021-31/01/2021
	730,524.54
	716,404.61
	0.00

	01/02/2021-28/02/2021
	1,709,427.65
	1,677,364.41
	0.00

	01/03/2021-31/03/2021
	1,892,953.75
	1,857,270.02
	0.00

	01/04/2021-30/04/2021
	1,830,882.93
	1,795,916.19
	0.00

	01/05/2021-31/05/2021
	1,891,422.59
	1,855,635.63
	0.00

	01/06/2021-30/06/2021
	1,831,130.92
	1,796,266.75
	0.00

	01/07/2021-31/07/2021
	1,892,290.74
	1,856,403.23
	0.00

	01/08/2021-31/08/2021
	1,890,585.62
	1,854,959.31
	0.00

	01/09/2021-30/09/2021
	1,832,125.27
	1,796,968.11
	0.00

	01/10/2021-31/10/2021
	1,891,749.11
	1,856,057.29
	0.00

	01/11/2021-30/11/2021
	1,832,514.66
	1,798,056.93
	0.00

	01/12/2021-31/12/2021
	1,893,279.86
	1,857,643.32
	0.00

	01/01/2022-31/01/2022
	1,893,467.77
	1,857,490.35
	0.00

	01/02/2022-28/02/2022
	1,709,805.85
	1,677,206.54
	0.00

	01/03/2022-31/03/2022
	1,892,099.12
	1,856,460.93
	0.00

	Total
	26,614,260.38
	26,110,103.62
	0.00




	Measurement methods and procedures
	Monitored continuously, record hourly and saved automatically in the Data Collection System (DCS). The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month, so this parameter can be sourced from production record from DCS system.

	Monitoring frequency
	Continuously measured by flowmeter 1, flowmeter 2 and flowmeter 3 

	QA/QC procedures
	Total 27 flow meters were calibrated on 08/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	To calculated CH4 generated in the anaerobic digester in the project situation QCH4,y

	Additional comment
	For this monitoring period, all the biogas produced is used for power generation, no surplus biogas for the flaring system.




	Data/parameter
	ECPJ,j,y

	Unit
	MWh

	Description
	Quantity of electricity consumed by the project in year y

	[bookmark: _Hlk74926311]Source of data
	Electricity daily report

	Value(s) of monitored parameter
		period
	ECPJ,j,y (MWh)
	period
	ECPJ,j,y (MWh)

	20/01/2021-31/01/2021
	6.26231
	01/09/2021-30/09/2021
	16.16606

	01/02/2021-28/02/2021
	16.16046
	01/10/2021-31/10/2021
	16.14432

	01/03/2021-31/03/2021
	16.15350
	01/11/2021-30/11/2021
	16.17640

	01/04/2021-30/04/2021
	16.14886
	01/12/2021-31/12/2021
	16.14725

	01/05/2021-31/05/2021
	16.16436
	01/01/2022-31/01/2022
	16.16076

	01/06/2021-30/06/2021
	16.14563
	01/02/2022-28/02/2022
	16.16939

	01/07/2021-31/07/2021
	16.16980
	01/03/2022-31/03/2022
	16.15244

	01/08/2021-31/08/2021
	16.14637
	Total
	232.47




	Measurement methods and procedures
	Use electricity meters 1 installed in the 9 manure treatment plants. 
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity consumption is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity consumption. 

	Monitoring frequency
	Continuous measurement and daily recording

	QA/QC procedures
	Total 9 meters were calibrated on 11/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG596-2012” Electrical Meters for Measuring Alternating-current Electrical Energy” in China.
Please refer to Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	And during this monitoring period, most of the electricity consumed by the project came from the electricity generated by the biogas generated from the anaerobic fermentation process of the project, which is belongs to self-generated and self-consumed. Only a small amount of the electricity consumption of AWMSs were sourced from the grid company when the biogas generators were not operation. 
The quantity of electricity consumed by the project are crosschecked with grid statement issued by the power grid company, and the value is consistent.



	[bookmark: _Hlk74749965]Data/parameter
	TDLj,y

	Unit
	%

	Description
	Average technical transmission and distribution losses for providing electricity to source j in year y  

	Source of data
	Tool 05 (Version 03.0)” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”

	Value(s) of monitored parameter
	20

	Measurement methods and procedures
	Default value of 20% is applied, which is conservative according to tool” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”

	Monitoring frequency
	The value can be changed once the tool is updated.

	QA/QC procedures
	Default value of 20% is applied, which is the maximum value as per Methodology tool 05 Version 03.0 and conservative

	Purpose of data
	Calculation of project emission

	Additional comment
	N/A



	Data/parameter
	Vt,db

	Unit
	m³ dry gas/h 

	Description
	Volumetric flow of the gaseous stream in time interval t on a dry basis 

	Source of data
	Direct monitored by Flowmeters

	Value(s) of monitored parameter
	
	period
	Vt,db (m³ dry gas/h) monitored  by flow meter 1
	Vt,db (m³ dry gas/h) monitored  by flow meter 2
	Vt,db (m³ dry gas/h) monitored  by flow meter 3

	20/01/2021-31/01/2021
	2536.54
	2487.52
	0.00

	01/02/2021-28/02/2021
	2543.79
	2496.08
	0.00

	01/03/2021-31/03/2021
	2544.29
	2496.33
	0.00

	01/04/2021-30/04/2021
	2542.89
	2494.33
	0.00

	01/05/2021-31/05/2021
	2542.23
	2494.13
	0.00

	01/06/2021-30/06/2021
	2543.24
	2494.81
	0.00

	01/07/2021-31/07/2021
	2543.40
	2495.17
	0.00

	01/08/2021-31/08/2021
	2541.11
	2493.22
	0.00

	01/09/2021-30/09/2021
	2544.62
	2495.79
	0.00

	01/10/2021-31/10/2021
	2542.67
	2494.70
	0.00

	01/11/2021-30/11/2021
	2545.16
	2497.30
	0.00

	01/12/2021-31/12/2021
	2544.73
	2496.83
	0.00

	01/01/2022-31/01/2022
	2544.98
	2496.63
	0.00

	01/02/2022-28/02/2022
	2544.35
	2495.84
	0.00

	01/03/2022-31/03/2022
	2543.14
	2495.24
	0.00

	Average
	2543.14
	2494.93
	0.00




	Measurement methods and procedures
	Monitored continuously, record hourly and saved automatically in the Data Collection System (DCS). The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month, so this parameter can be sourced from “production record from DCS system”. 

	Monitoring frequency
	Continuous measurement 

	QA/QC procedures
	Total 27 flow meters were calibrated on 08/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Vi,t,db

	Unit
	m³ gas i/m³ dry gas 

	Description
	Volumetric fraction of greenhouse gas i in a time interval t on a dry basis 

	Source of data
	Monitored by gas analyzers

	Value(s) of monitored parameter
		period
	Vi,t,db
	period
	Vi,t,db

	20/01/2021-31/01/2021
	60.84
	01/09/2021-30/09/2021
	60.60

	01/02/1021-28/02/2021
	60.99
	01/10/2021-31/10/2021
	60.71

	01/03/2021-31/03/3021
	61.13
	01/11/2021-30/11/2021
	60.68

	01/04/2021-30/04/2021
	61.00
	01/12/2021-31/12/2021
	61.36

	01/05/2021-31/05/2021
	61.38
	01/01/2022-31/01/2022
	61.30

	01/06/2021-30/06/2021
	61.23
	01/02/2022-28/02/2022
	61.54

	01/07/2021-31/07/2021
	60.77
	01/03/2022-31/03/2022
	60.11

	01/08/2021-31/08/2021
	60.89
	Average
	60.97




	Measurement methods and procedures
	Measured continuously and record hourly by online gas analysers installed at the outlet of the anaerobic digesters and saved automatically in the DCS (Data Collection System).
The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month. Daily and Monthly CH4 concentration was calculated based on the 24-hour average and daily average CH4 concentration.

	Monitoring frequency
	Continuous measurement   

	QA/QC procedures
	All the gas analysers were calibrated on 08/01/2021 and 06/01/2022 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG693-2011” Verification Regulation of Alarmer Detectors of Combustible Gas” in China. And the zero verification with an inert gas (N2) and one reading verification with a standard gas (single calibration gas) are implemented in the process of calibration, which is in accordance with JJG693-2011. All calibration gases are from Nanjing Changyuan Industrial Gas Co.Ltd, which is a qualified reference materials manufacturer issued by the General Administration of Quality Supervision, Inspection and Quarantine of the People's Republic of China on 06/09/2017.
Please refer to Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Tt

	Unit
	K 

	Description
	Temperature of the gaseous stream in time interval t 

	Source of data
	Measured by instrument and recorded in production record

	Value(s) of monitored parameter
		period
	Tt
	period
	Tt

	20/01/2021-31/01/2021
	309.53
	01/09/2021-30/09/2021
	309.57

	01/02/1021-28/02/2021
	309.42
	01/10/2021-31/10/2021
	309.98

	01/03/2021-31/03/3021
	309.25
	01/11/2021-30/11/2021
	309.62

	01/04/2021-30/04/2021
	309.08
	01/12/2021-31/12/2021
	309.62

	01/05/2021-31/05/2021
	310.01
	01/01/2022-31/01/2022
	309.71

	01/06/2021-30/06/2021
	309.25
	01/02/2022-28/02/2022
	309.78

	01/07/2021-31/07/2021
	309.67
	01/03/2022-31/03/2022
	310.34

	01/08/2021-31/08/2021
	309.76
	Average
	309.64




	Measurement methods and procedures
	Measured continuously by the biogas flow meters, since the flowmeters can monitor other parameter such as Vt,db, Tt and Pt simultaneously. And record hourly and saved automatically in the DCS system. The readout of flowmeter was indicated degrees Celsius (°C). Therefore, the temperature Tt(K) is calculated as the equation T(K)=t(°C) +273.15
The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month. Daily and Monthly temperature was calculated based on the 24-hour average and daily average temperature.

	Monitoring frequency
	Continuous measurement

	QA/QC procedures
	Total 27 flow meters were calibrated on 08/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Pt

	Unit
	Pa 

	Description
	Pressure of the gaseous stream in time interval t 

	Source of data
	Measured by instrument and recorded in production record

	Value(s) of monitored parameter
		period
	Pt
	period
	Pt

	20/01/2021-31/01/2021
	101325
	01/09/2021-30/09/2021
	101325

	01/02/1021-28/02/2021
	101325
	01/10/2021-31/10/2021
	101325

	01/03/2021-31/03/3021
	101325
	01/11/2021-30/11/2021
	101325

	01/04/2021-30/04/2021
	101325
	01/12/2021-31/12/2021
	101325

	01/05/2021-31/05/2021
	101325
	01/01/2022-31/01/2022
	101325

	01/06/2021-30/06/2021
	101325
	01/02/2022-28/02/2022
	101325

	01/07/2021-31/07/2021
	101325
	01/03/2022-31/03/2022
	101325

	01/08/2021-31/08/2021
	101325
	Average
	101325




	Measurement methods and procedures
	Measured continuously by the biogas flow meters since the flowmeters can monitor other parameter such as Vt,db, Tt and Pt simultaneously. And record hourly and saved automatically in the DCS system. The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month. Daily and Monthly temperature was calculated based on the 24-hour average and daily average temperature.

	Monitoring frequency
	Continuous measurement

	QA/QC procedures
	Total 27 flow meters were calibrated on 08/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	

	Unit
	kg gas i/m³ gas i

	Description
	Density of greenhouse gas i in the gaseous stream in time interval t 

	Source of data
	Calculated 

	Value(s) of monitored parameter
		period
	
	period
	

	20/01/2021-31/01/2021
	0.00063
	01/09/2021-30/09/2021
	0.00063

	01/02/1021-28/02/2021
	0.00063
	01/10/2021-31/10/2021
	0.00063

	01/03/2021-31/03/3021
	0.00063
	01/11/2021-30/11/2021
	0.00063

	01/04/2021-30/04/2021
	0.00063
	01/12/2021-31/12/2021
	0.00063

	01/05/2021-31/05/2021
	0.00063
	01/01/2022-31/01/2022
	0.00063

	01/06/2021-30/06/2021
	0.00063
	01/02/2022-28/02/2022
	0.00063

	01/07/2021-31/07/2021
	0.00063
	01/03/2022-31/03/2022
	0.00063

	01/08/2021-31/08/2021
	0.00063
	Average
	0.00063




	Measurement methods and procedures
	Calculated based on temperature of the gaseous stream in time interval t and pressure of the gaseous stream in time interval t.

	Monitoring frequency
	Pressure and temperature are measured continuously by the biogas flow meters 

	QA/QC procedures
	Calculated value according to the pressure and temperature

	Purpose of data
	Calculation of project emissions

	Additional comment
	NA



	[bookmark: _Hlk88209644]Data/parameter
	MS%j

	Unit
	Fraction

	Description
	Fraction of manure handled in system j in project activity

	Source of data
	PDD

	Value(s) of monitored parameter
	[bookmark: OLE_LINK33]100%. As this parameter is not monitored during this monitoring period. so, to be conservative, the value of this parameter in the emission reduction calculation is 100%, which is consistent with PDD.

	Measurement methods and procedures
	All the manure flew into AWMSs to be treated, therefore, value of 100% is applied.

	Monitoring frequency
	Annually

	QA/QC procedures
	All the manure flew into AWMSs to be treated; no any manure will be discharged outside. Therefore, the value of this parameter is 100%.

	Purpose of data
	Calculation of project emissions

	Additional comment
	NA



	[bookmark: _Hlk95291447]Data/parameter
	B0, LT

	Unit
	m3CH4/kg -dm

	Description
	Maximum methane producing potential of the volatile solid generated by animal type LT 

	Source of data
	IPCC 2006 table 10A-7 and 10A-8, chapter 10, volume 4 

	Value(s) applied
	B0, LT (Market swine) =0.29[footnoteRef:7] [7:  The project is located in Guaingxi Zhuang Autonomous Region, China, Asia. According to Table 10A-7 and 10A-8 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10, the maximum methane producing potential(B0,LT) for Market swine and Breeding swine in Asia region is 0.29 m3 CH4/kg VS.] 

B0, LT (Breeding swine) =0.29

	Measurement methods and procedures  
	B0, LT can be measured as per ISO 11734:1995. As this parameter is not monitored in the actual operation. so, in the monitoring period 0.29 m3CH4/kg -dm is still applied. While the actual methane producing potential of the volatile solid generated by swine manure is 479.4ml/g VS according to the public literature[footnoteRef:8],which is higher. Therefore 0.29 m3CH4/kg -dm applied in monitoring period is conservative. [8:  http://www.doc88.com/p-9902182440715.html] 


	Monitoring frequency
	Annually

	QA/QC procedures
	The value is taken from published sources. The parameter value should be updated on latest available public data source.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	 N/A



	Data/parameter
	NEXLT,y

	Unit
	kg N/animal/year 

	Description
	Annual average nitrogen excretion per head of a defined livestock population estimated as described in Appendix 2

	Source of data
	Calculated as the equation of option 2 in Appendix 2: 

While, NEXIPCC default calculated as equation 30 of the IPCC 2006, volume 4, chapter 10
NEXIPCC default =Nrate(T)* TAM/1000*365

	Value(s) applied
		Period
	Market swine
	Breeding swine

	20/01/2021-31/01/2021
	0.31
	0.23

	01/02/2021-28/02/2021
	0.72
	0.52

	01/03/2021-31/03/2021
	0.81
	0.58

	01/04/2021-30/04/2021
	0.78
	0.56

	01/05/2021-31/05/2021
	0.80
	0.58

	01/06/2021-30/06/2021
	0.77
	0.56

	01/07/2021-31/07/2021
	0.80
	0.58

	01/08/2021-31/08/2021
	0.81
	0.58

	01/09/2021-30/09/2021
	0.78
	0.56

	01/10/2021-31/10/2021
	0.80
	0.58

	01/11/2021-30/11/2021
	0.76
	0.56

	01/12/2021-31/12/2021
	0.80
	0.58

	01/01/2022-31/01/2022
	0.79
	0.59

	01/02/2022-28/02/2022
	0.72
	0.52

	01/03/2022-31/03/2022
	0.81
	0.58





	Measurement methods and procedures  
	Nrate(T) and TAM are default value from IPCC 2006

	Monitoring frequency
	Annually

	QA/QC procedures
	The parameter is calculated as the equation of option 2 in Appendix 2 and the value of other parameter applied in the equation is taken from published sources (2006 IPCC). The value should be updated on latest available public data source.

	Purpose of data
	Baseline, Project and leakage emissions calculations

	Additional comment
	N/A



	[bookmark: _Hlk95291461]Data/parameter
	Type

	Unit
	 /

	Description
	Type of barn and AWMS  

	Source of data
	Project proponent

	Value(s) applied
	NA

	Measurement methods and procedures  
	The swine barn and AWMS layout and configuration are collected. Archive electronically during project plus 5 years.

	Monitoring frequency
	Once for each monitoring period

	QA/QC procedures
	After the first verification, only changes in the type of barn and AWMS will be reported. 

	Purpose of data
	Confirm whether the implementation of project as design 

	Additional comment
	Swine barn and AWMS layout and configuration.



	[bookmark: _Hlk95291479]Data/parameter
	T

	Unit
	 °C

	Description
	Annual average ambient temperature at project site

	Source of data
	Publicly available data

	Value(s) applied
		Year
	T(°C)

	2021
	21.6

	2022
	NA[footnoteRef:9] [9:  This monitoring period only includes the first 3 months of 2022 year and the temperature in first 3 months cannot represent the whole 2022 year, so the annual average temperature in 2022 is not yet available. So, in this monitoring period, the Annual average ambient temperature at project site of 2022 applied the value of 2021.] 





	Measurement methods and procedures  
	The average  project site temperature in 2021 is 21.6℃, which is which is sourced from  Guangxi Meteorological Observatory[footnoteRef:10],[footnoteRef:11].  [10:  http://gx.sina.com.cn/news/gx/2022-01-09/detail-ikyakumx9216825.shtml]  [11:  http://gx.cma.gov.cn/] 


	Monitoring frequency
	monthly

	QA/QC procedures
	After comparing the actual temperature 21.6℃ and the temperature of ex-ante estimated(17.5~23.5℃),  So, in this monitoring period, MCFj value is 76% with the lower temperature of 17.5°C as per Appendix 3 of ACM0010(Version 08.0). Then multiplying MCF values with a value of 0.94, so 71.44% of MCFj is used for calculation during in this monitoring period.

	Purpose of data
	Used to select the annual MCFj from IPCC 2006 Guidelines

	Additional comment
	NA 



SDG 7
	Data / Parameter
	EGd,y

	Unit
	MWh

	Description
	Total electricity produced

	Source of data
	Direct measurement

	Value(s) of monitored parameter
		period
	EGd,y(MWh)

	20/01/2021-31/01/2021
	922.96276

	01/02/2021-28/02/2021
	2,159.82626

	01/03/2021-31/03/2021
	2,391.71629

	01/04/2021-30/04/2021
	2,313.26101

	01/05/2021-31/05/2021
	2,389.75183

	01/06/2021-30/06/2021
	2,313.60006

	01/07/2021-31/07/2021
	2,390.86914

	01/08/2021-31/08/2021
	2,388.70687

	01/09/2021-30/09/2021
	2,314.85287

	01/10/2021-31/10/2021
	2,390.19337

	01/11/2021-30/11/2021
	2,315.34023

	01/12/2021-31/12/2021
	2,392.14162

	01/01/2022-31/01/2022
	2,392.35936

	01/02/2022-28/02/2022
	2,161.06251

	01/03/2022-31/03/2022
	2,391.46921

	Total
	33628.11




	Measurement methods and procedures
	Use electricity meters 2 installed at the outlet of biogas generator. 
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity generation is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity generation.

	Monitoring frequency
	Continuous measurement and daily recording

	QA/QC procedures
	total 9 meters were calibrated on 11/01/2021 by Guangxi Zhuang Autonomous Region Institute of Metrology and testing in compliance with JJG596-2012” Electrical Meters for Measuring Alternating-current Electrical Energy” in China.
Please refer to Section C of the MR for more details.

	Purpose of data
	To demonstrate contribution to SDG 7.

	Additional comment
	N/A



SDG 8
	Data / Parameter
	Total number of jobs 

	Unit
	Number of full-time jobs created

	Description
	Full-time Jobs created for both men and women.

	Source of data
	Record keeping book 

	Value(s) of monitored parameter
	18 full-time jobs are created including 9 males and 9 females 

	Measurement methods and procedures
	Source of data was record keeping book and was cross checked by the labor contracts.

	Monitoring frequency
	annually.

	QA/QC procedures
	After the first verification, only changes in employees will be reported.
The results shall be cross checked with labor contract.

	Purpose of data
	To demonstrate contribution to SDG 8.

	Additional comment
	N/A


[bookmark: _Hlk75163211]
Mitigation Measure for Safeguarding Principles
	Data / Parameter
	Employee Training of biogas safety operation

	Unit
	/

	Description
	Employees was trained on the safety operation of the biogas 

	Source of data
	Training notice 

	Value(s) of monitored parameter
	Training for the biogas safety operation was held on 15/12/2020 and 13/12/2021

	Measurement methods and procedures
	Training once a year
The training content includes basic biogas knowledge, Operating condition control, operating procedure, patrol inspection, Operation management and failure process. All 18 staffs from 9 swine farms attended this training. 
All staff strictly follow the operation procedures in the process of operation and there are no safety accidents occurred during this monitoring period. Therefore, the training is effective.

	Monitoring frequency
	once a year

	QA/QC procedures
	Meeting attendance record was used to cross-checked.

	Purpose of data
	To demonstrate Mitigation Measure for Safeguarding Principles

	Additional comment
	N/A



[bookmark: _Toc341456040][bookmark: _Toc40962778]Comparison of monitored parameters with last monitoring period
NA. This is the 1st monitoring period, no last monitoring period can be compared.

Implementation of sampling plan
>>
According to the PDD, the sample size is calculated according to the design scale and fixed during the monitoring period. During this monitoring period, the sampling is implemented according to the stratified sampling method for the monitoring of Wsite described in Section C of MR. The detailed steps are as following:
1. the overall sample size based on the design population of swine firstly is calculated. 
2. As the project involved 9 swine farms, then the sample size in each swine farm is adjusted based on the proportion of the number of each farm in the total number of 9 farms. 
3. Similarly, the sample size of each age group of Market swine and Breeding swine in each farm is also calculated based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in the farm. 
4. After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample is conducted in every swine farm. Since swine in different age are kept in the different swine houses, samples can be randomly selected from swine houses of this age group. 
5. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. 
6. The sample will be marked after weighting and if the sample swine is still drawn next month, then this sample swine needs to be discarded and a new sample swine is drawn, this will be done every month until the end of the monitoring period.

Step 1. overall sample size calculation 
According to “Standard: Sampling and surveys for CDM project activities and programmes of activities (Version 09.0)”, the desired confidence level is 95% and the desired precision is 10%. According to statistical principles and sampling survey method, 422 samples should be sufficient to satisfy the desired confidence and precision. For mean value sampling, the required sampling quantity is calculated by the following steps:


n2= n1N/(N+n1)
n3=Bn2
n4= n3/r
n= n4 (110%) 
Where:
Z    the Z-statistic and the value taken is 1.96 (corresponding to 90% confidence level);
σ   the standard deviation;
d   the maximum error of estimate;
X   the mean value of samples;
V   the coefficient of variation, V= σ/X≤1 and its maximum value 1 is taken;
e   the allowed relative sampling error (“precision”) and the value taken is 10% 
N   the total number of swine population 259,710[footnoteRef:12];  [12:  According to PDD, this value is the total of population of animals in the farms, including market swine and breeding swine. 
] 

B   the survey design effect and the B value taken is 1 because for stratification sampling the B value is less than or equal to 1;
r    the survey reply rate and the value taken is 100%; 
110%  10% contingency was added to produce the final sample size; 
n1, n2, n3, n4, n  the adjusted values after each step with n being the final number of samples to be taken. Actually, n4 is the required number of samples based on calculation, 10% contingency was added to n4 to produce n in this sampling.
	[bookmark: _Hlk56001304]Z
	V
	e
	N
	B
	r

	1.96
	1
	10%
	259,710
	1
	100%

	n1
	
	384

	n2
	n1N/(N+n1)
	384

	n3
	Bn2
	384

	n4
	n3/r
	384

	n
	n4 (110%)
	422



Step 2 adjust sample size based on the proportion of the number of each farm in the total number of 9 farms
Stratified sampling (with samples of 422) was used for the monitoring of Wsite. However, the samples number in the nine subsidiary farms is decimals according to the proportion of the number of each farm in the total number of 9 farms. To be conservative, both the samples number of the 9 subsidiary farms is adjusted to be integer value. As a result, 429 samples of swine population were selected within the project boundary using Excel to ensure conservation. 
The distribution of the samples in each swine farm shows as follow:
	[bookmark: _Hlk56001479]Swine farm
	Sample size

	
	Market swine
	Breeding swine

	Bama Yanyan swine farm
	36 
	22 

	Chongzuo Zuozhou swine Farm
	20 
	12 

	Tianyang Wucun swine Farm
	17 
	11 

	Quanzhou Dengjiabu swine Farm
	10 
	6 

	Chongzuo Quming swine Farm
	39 
	24 

	Jingxi swine Farm
	45 
	28 

	Liucheng Mashan swine Farm
	59 
	36 

	Tengxian Tianping swine Farm
	30 
	18 

	Debao Chengguan swine Farm
	16 
	0 

	Total
	429



Step 3 Determine sample size based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in two kinds of farms.
According to the methodology ACM0010, each defined livestock population should be classified into a minimum of three age categories. Nursery phase, Growing phase and Mature phase in fattening farms and breeding farms was be selected through the proportion of swine population in three age categories during this monitoring period. At the same time, to be conservative, both the samples number of the three age categories is adjusted to be integer value.
In conclusion, 444 samples of swine population are fixed and the distribution of the samples for three age categories in each swine farm shows as follow:
The distribution of the samples in each age group of Market and Breeding swine in each farm:
	[bookmark: _Hlk56001316]Swine farm
	Market swine
	Breeding swine 

	
	Nursery phase
	Growing phase
	Mature phase
	Nursery phase
	Growing phase
	Mature phase

	Bama Yanyan swine farm
	12
	12
	12
	8
	8
	8 

	Chongzuo Zuozhou swine Farm
	7
	7
	7
	4
	4
	4 

	Tianyang Wucun swine Farm
	6
	6
	6
	4
	4
	4 

	Quanzhou Dengjiabu swine Farm
	4
	4
	4
	2
	3
	3 

	Chongzuo Quming swine Farm
	13
	13
	13
	8
	8
	8 

	Jingxi swine Farm
	15
	15
	15
	10
	10
	10 

	Liucheng Mashan swine Farm
	20
	20
	20
	12
	12
	12 

	Tengxian Tianping swine Farm
	10
	10
	11
	6
	6
	6 

	Debao Chengguan swine Farm
	6
	6
	6
	0
	0
	0 

	Total
	444



Step 4 sampling and measure
After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample and measure are conducted in every swine farm. Since swine in different age are kept in the different pig houses, samples can be randomly selected from pig houses of this age group. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. If the same sample is taken in the following month, then a new sample was taken. This was done every month until the end of the monitoring period. 

For this monitoring period, then samples are selected randomly from pig houses of this age group by the technicians in the swine farms and then be measured by weight measures in the end of each month. At the same time, the measured value is recorded in the weight record table by the technicians in the swine farms.

At last, the monthly average Wsite of market swine and breeding swine was calculated by weighted the Wsite of all market swine sample and breeding swine sample. 

The Monitoring Team implemented the sampling investigation strictly follow the guidance. The monitoring data was collected throughout the entire crediting period of the project.

According to Standard: Sampling and surveys of CDM project activities and programmes of activities (Version 09.0), confidence/precision have been calculated and checked as follows:

1. The stratified estimated overall mean
The sample estimate of the overall mean operation hour is calculated with the equation below:(1)


Where:
mStrat  The stratified estimated overall mean
gi  Size of the ith district where i=a,…,k
N  Population total 
mi  Mean of the ith district where i=a,…,k

2. The standard error of the stratified estimated overall mean
The standard error of the stratified estimated overall mean is calculated as follows:(2)


Where:
s.e.(mStrat)  Standard error of the stratified estimated overall mean
gi  Size of the ith district where i=a,…,k
N  Population total 
ni  Number of sampled units the ith district where i=a,…,k
SDi2  Variance of the ith district where i=a,…,k

3. t-value
t-value is depending on:
(i) The level of confidence, and
(ii) The size of the sample.
The t-value associated with 95% confidence and the sample size of 444 is 1.9653 as derived in Microsoft Excel using the TINV function.

4. Precision
The precision associated with an estimate is:
t-value × standard error of the mean

5. Calculation results
[bookmark: _Hlk63427774]For Wsite, according to “Standard: Sampling and surveys for CDM project activities and programmes of activities (Version 09.0)”, the desired confidence level is 95% and the desired precision is 10%. According to statistical principles and sampling survey method, 444 samples should be sufficient to satisfy the desired confidence and precision.
[bookmark: _Hlk63427796]The calculation results are shown below. For more details of these calculations, please refer to the ER calculation spread sheet.
	time
	t-value
	mStrat
	s.e. (mStrat)
	Precision
	Relative Precision

	20/01/2021-31/01/2021
	1.9653 
	64.77 
	1.25 
	2.4480 
	3.78%

	01/02/1021-28/02/2021
	1.9653 
	50.21 
	1.11 
	2.1871 
	4.36%

	01/03/2021-31/03/3021
	1.9653 
	51.20 
	1.15 
	2.2646 
	4.42%

	01/04/2021-30/04/2021
	1.9653 
	50.91 
	1.12 
	2.1972 
	4.32%

	01/05/2021-31/05/2021
	1.9653 
	50.91 
	1.12 
	2.2104 
	4.34%

	01/06/2021-30/06/2021
	1.9653 
	50.41 
	1.13 
	2.2302 
	4.42%

	01/07/2021-31/07/2021
	1.9653 
	50.46 
	1.14 
	2.2312 
	4.42%

	01/08/2021-31/08/2021
	1.9653 
	50.63 
	1.15 
	2.2559 
	4.46%

	01/09/2021-30/09/2021
	1.9653 
	50.72 
	1.16 
	2.2809 
	4.50%

	01/10/2021-31/10/2021
	1.9653 
	50.60 
	1.16 
	2.2762 
	4.50%

	01/11/2021-30/11/2021
	1.9653 
	50.11 
	1.11 
	2.1822 
	4.36%

	01/12/2021-31/12/2021
	1.9653 
	50.80 
	1.15 
	2.2562 
	4.44%

	01/01/2022-31/01/2022
	1.9653 
	50.52 
	1.13 
	2.2209 
	4.40%

	01/02/2022-28/02/2022
	1.9653 
	50.55 
	1.12 
	2.1972 
	4.35%

	01/03/2022-31/03/2022
	1.9653 
	50.36 
	1.12 
	2.2030 
	4.37%



[bookmark: _Hlk63428020]In conclusion, the 444 samples are sufficient to satisfy the desired confidence and precision.



SECTION E. [bookmark: _Toc315189228][bookmark: _Toc317860226][bookmark: _Toc341474081][bookmark: _Toc40962779][bookmark: _Ref47706333][bookmark: _Ref49860683]CALCULATION OF SDG IMPACTS
[bookmark: _Ref315873983][bookmark: _Ref418095428][bookmark: _Toc40962780]Calculation of baseline value or estimation of baseline situation of each SDG Impact
>>
SDG 7 Impact of baseline situation
Total electricity produced from 20/01/2021 to 31/12/2021 in baseline situation is 0 MWh.
Total electricity produced from 01/01/2022 to 31/03/2022 in baseline situation is 0 MWh.
In baseline scenario, 0 MWh electricity produced from 20/01/2021 to 31/03/2022.

SDG 8 Impact of baseline situation
From 20/01/2021 to 31/12/2021, 0 full-time jobs created in the baseline situation.
From 01/01/2022 to 31/03/2022, 0 full-time jobs created in the baseline situation.
Without the project activity, 0 full-time jobs created during the 1st monitoring period from 20/01/2021 to 31/03/2022.

SDG 13 Impact of baseline situation
From 20/01/2021 to 31/12/2021, the amount of GHGs emission avoided or sequestered in baseline is 0 tCO2e.
From 01/01/2022 to 31/03/2022, the amount of GHGs emission avoided or sequestered in baseline is 0 tCO2e.
Without the project activity, the amount of GHGs emission avoided or sequestered in this monitoring period is 0 tCO2e.

[bookmark: _Ref315873986][bookmark: _Ref418095432][bookmark: _Toc40962781]Calculation of project value or estimation of project situation of each SDG Impact
>>
SDG 7 Impact of project situation
Total electricity produced from 20/01/2021 to 31/12/2021 in project situation is 26,683.22 MWh. 
Total electricity produced from 01/01/2022 to 31/03/2022 in project situation is 6,944.89MWh. 
For this monitoring period from 20/01/2021 to 31/03/2022, total electricity produced is 33,628.11MWh.

SDG 8 Impact of project situation
From 20/01/2021 to 31/12/2021, 18 full-time jobs created (including 9 females and 9 males).
From 01/01/2022 to 31/03/2022, 18 full-time jobs created (including 9 females and 9 males).
For the 1st monitoring period from 20/01/2021 to 31/03/2022, 18 full-time jobs created (including 9 females and 9 males).

SDG 13 Impact of project situation
As per section B.6.1 of the PDD, in project situation, the amount of GHGs emissions avoided or sequestered can be obtained by baseline emission – project emissions – leakage emissions, and the baseline emission, project emissions, leakage emissions can be determined by ACM0010” GHG emission reductions from manure management systems (Version 08.0)”, the specific calculation method and calculation result in this monitoring period are described as follows.
Baseline emission
As per section B.6 of the PDD, baseline emissions in year y (BEy) can be calculated as follows,
Baseline emissions are：
        (Equation 1)

where:
	BEy
	Baseline emissions in year y (t CO2/yr)

	BECH4, y
	Baseline CH4 emissions in year y (t CO2/yr)

	BEN2O, y
	Baseline N2O emissions in year y (t CO2/yr)

	BEelec/heat,y
	Baseline CO2 emissions from electricity and/or heat used in the baseline (t CO2/yr) 


i) Baseline CH4 emissions (BECH4, y)
    (Equation 2)
where:
	BECH4, y
	Baseline CH4 emissions in year y (t CO2/yr)

	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/t CH4) 

	DCH4
	Density of CH4 (t/m3). 0.00067t/m3 at room temperature(20℃)and 1am pressure.

	MCFj
	Annual methane conversion factor (MCFj) for the baseline AWMSj. IPCC 2006, Table 10.17, chapter 10, volume 4.

	B0,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg-dm) 

	NLT
	Annual average number of animals of type LT for the year y (number)

	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr)

	MS%Bl,j
	Fraction of manure handled in system j in the baseline. In this project, the baseline manure management system is uncovered anaerobic lagoon only. The amount of manure handled by the anaerobic lagoon is 100%. MS%Bl,j =100% 

	LT
	Type of livestock 

	j
	Type of treatment system 



Estimation of various variables and parameters for above equations:
(A) As per PDD, VSLT,y shall be determined in following way.

Scaling default IPCC values VSdefault to adjust for a site-specific average animal weight as shown in equation below:
                      (Equation 3)
where:
	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr) 

	Wsite
	Average animal weight of a defined livestock population at the project site (kg) 

	Wdefault
	Default average animal weight of a defined population (kg) 

	VSdefault
	Default value for the volatile solid excretion per day on a dry-matter basis for a defined livestock population (kg-dm/animal/day) 

	ndy
	Number of days treatment plant was operational in year y 


 
(B)Annual average number of animals of type LT (NLT) shall be determined in following ways
Option 1:
          (Equation 4)
where:
	NLT
	Annual average number of animals of type LT for the year y (number) 

	Nda,LT
	Number of days animal of type LT is alive in the farm in the year y (number) 

	Np,LT
	Number of animals of type LT produced annually for the year y (number) 



Option 2:
If the project developer can monitor in a reliable and traceable way the daily stock of animals in the farm, discounting dead animals and animals discarded from the productive process from the daily stock, then the annual average number of animals (NLT) may be calculated as follows: 
     (Equation 5)
where:
	NLT
	Annual average number of animals of type LT for the year y (number) 

	NAA,LT
	Daily stock of animals of type LT in the farm, discounting dead and discarded animals (number) 



[bookmark: OLE_LINK4]There are two types of swine in this project, i.e., Market swine and Breeding swine. For Market swine, Option 1 is adopted to calculate NLT. For Breeding swine, the PP can monitor the daily stock of breeding swine in a reliable way, discounting dead breeding swine and discarded them from the productive process from the daily stock. So, the Option 2 is adopted to calculate NLT for Breeding swine. 

(C) Maximum methane producing potential(B0,LT)
According to applied methodology ACM0010(Version 08.0), this value varies by species and diet. Default values are used, and they are taken from tables 10A-4 through 10A-9 (IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10).

The proposed project is located in Guangxi Province, China, Asia. According to Table 10A-7 and 10A-8 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10, the maximum methane producing potential(B0,LT) for Market swine and Breeding swine in Asia region is 0.29 m3 CH4/kg VS.

(D) Annual methane conversion factor (MCFj) for the baseline AWMSj
(a)The MCFj values given in Table 10.17, chapter 10, volume 4, IPCC 2006 Guidelines should be used. MCFj values depend on the annual average temperature where the anaerobic manure treatment facility in the baseline existed. For this project, the annual average temperature in this monitoring period is 21.6 ℃, while the average temperature in ex-ante estimated is 17.5~23.5 ℃, so the value of 76% is applied in this monitoring period.
(b)A conservativeness factor should be applied by multiplying MCFj values (estimated as per above bullet) with a value of 0.94, to account for the 20% uncertainty in the MCFj values as reported by IPCC 2006.

ii)Baseline N2O emissions (BEN2O,y)
        (Equation 6)
where：
	BEN2O,y
	Annual baseline N2O emissions in (t CO2e/yr) 

	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O) 

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28) 

	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/year) 

	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 



              (Equation 7)
where：
	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/yr) 

	EFN2O,D,j
	Direct N2O emission factor for the treatment system j of the manure management system (kg N2O-N/kg N). (Estimated with site-specific, regional or national data if such data is available, otherwise use default EF3 from Table 10.21, chapter 10, volume 4, in the IPCC 2006 Guidelines for National Greenhouse Gas Inventories). The site-specific, regional or national data are not available, so this project activity adopts default EF3.

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in Appendix 2 

	MS%Bl,j
	Fraction of manure handled in system j (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



                   (Equation 8)
where:
	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 

	EFN2O,ID
	Indirect N2O emission factor for N2O emissions from atmospheric deposition of nitrogen on soils and water surfaces (kgN2O-N/kg NH3-N and NOX-N). (Estimated with site-specific, regional or national data if such data is available. Otherwise, default values for EF4 from Table 11.3, chapter 11, volume 4 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories
can be used). The site-specific, regional or national data are not available, so this project activity adopts default EF4.

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%Bl,j
	Fraction of manure handled in system j (fraction) 

	FgasMS,j,LT
	Default values for nitrogen loss due to volatilisation of NH3 and NOX from manure management (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



Estimation of various variables and parameters for above equations:
(A) As per PDD, the procedure for estimating NEXLT,y  in following way:
In the absence of availability of project specific information on protein intake, which should be justified in the “CDM-PDD”, national or regional data should be used for the nitrogen excretion NEXLT,y, if available. In the absence of such data, default values from Table 10.19 of the IPCC 2006, volume 4, chapter 10) may be used and should be corrected for the animal weight at the project site in the following way: 
                     (Equation 9)
where:
	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) 

	Wsite
	Average animal weight of a defined livestock population at the project site (kg) 

	Wdefault
	Default average animal weight of a defined population (kg) 

	NEX IPCC default
	Default value for the nitrogen excretion per head of a defined livestock population (kg N/animal/year) 



                (Equation 10)
where:
	Nrate(T)
	the default N excretion rate, kg N/ (1000 kg animal mass)/ day, Table 10.19, chapter 10, volume 4 of IPCC 2006 Guidelines

	TAM
	Typical animal mass for livestock in kg/animal



Table 8 data of parameter
	Time
	NLT
	NAA,LT
	Wsite (kg)
	VSLT,y (kg-dm/ animal/year)
	ndy(day)
	NEXIPCC (kg N/animal/year)
	NEXLT,y (kg N/animal/year)

	
	Market swine
	Breeding swine
	Market swine
	Breeding swine
	Market swine
	Breeding swine
	
	Market swine
	Breeding swine
	Market swine
	Breeding swine

	20/01/2021-31/01/2021
	152,825
	89,885
	60.8
	79.6
	7.82
	10.23
	12
	0.14
	0.08
	0.31
	0.23

	01/02/2021-28/02/2021
	152,825
	89,832
	61.6
	77.1
	18.48
	23.13
	28
	0.33
	0.19
	0.72
	0.52

	01/03/2021-31/03/2021
	152,825
	89,845
	62.2
	77.5
	20.66
	25.74
	31
	0.36
	0.21
	0.81
	0.58

	01/04/2021-30/04/2021
	152,825
	89,915
	62.2
	78.0
	19.99
	25.07
	30
	0.35
	0.20
	0.78
	0.56

	01/05/2021-31/05/2021
	152,825
	89,809
	61.3
	78.5
	20.36
	26.07
	31
	0.36
	0.21
	0.80
	0.58

	01/06/2021-30/06/2021
	152,825
	89,754
	61.3
	77.8
	19.70
	25.01
	30
	0.35
	0.20
	0.77
	0.56

	01/07/2021-31/07/2021
	152,825
	89,905
	61.3
	77.9
	20.36
	25.87
	31
	0.36
	0.21
	0.80
	0.58

	01/08/2021-31/08/2021
	152,825
	89,670
	62.1
	78.1
	20.63
	25.94
	31
	0.36
	0.21
	0.81
	0.58

	01/09/2021-30/09/2021
	152,825
	89,854
	61.6
	77.5
	19.80
	24.91
	30
	0.35
	0.20
	0.78
	0.56

	01/10/2021-31/10/2021
	152,825
	89,790
	61.4
	77.4
	20.39
	25.71
	31
	0.36
	0.21
	0.80
	0.58

	01/11/2021-30/11/2021
	152,825
	89,905
	60.6
	77.5
	19.48
	24.91
	30
	0.35
	0.20
	0.76
	0.56

	01/12/2021-31/12/2021
	152,825
	89,761
	61.7
	77.5
	20.49
	25.74
	31
	0.36
	0.21
	0.80
	0.58

	01/01/2022-31/01/2022
	152,825
	89,894
	60.4
	79.4
	20.06
	26.37
	31
	0.36
	0.21
	0.79
	0.59

	01/02/2022-28/02/2022
	152,825
	89,820
	61.6
	77.9
	18.48
	23.37
	28
	0.33
	0.19
	0.72
	0.52

	01/03/2022-31/03/2022
	152,825
	89,703
	62.0
	77.9
	20.59
	25.87
	31
	0.36
	0.21
	0.81
	0.58






Table 9 The calculation result of BECH4,y
	Parameter
	Value　
	Unit

	species
	Market Swine
	Breeding Swine
	

	GWPCH4
	28
	28
	tCO2/tCH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFj
	76%
	76%
	%

	Conservative Factor
	0.94
	0.94
	/　

	MCF with cons. Factor
	0.7144
	0.7144
	/　

	Bo,LT
	0.29
	0.29
	m3 CH4 /kg-dm

	NLT
	 Refer to Table 8

	Wsite
	 Refer to Table8

	Wdefault
	28
	28
	kg

	VSdefault
	0.3
	0.3
	Kg-dm/animal/day

	VSLT,y
	Refer to Table 8

	MS%Bl,j
	100%
	100%
	%

	ndy
	Refer to Table8

	BECH4,y in 20/01/2021-31/12/2021
	236,176
	tCO2e

	BECH4,y in 01/01/2022-31/03/2022
	61,514
	tCO2e

	BECH4,y
	297,690
	tCO2e



Table 10 The calculation result of BEN2O,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	EFN2O,D,j
	0
	0
	kg N2O-N/kg N

	EFN2O,ID,j
	0.01
	0.01
	kg N2O-N/kg N

	Nrate(T)
	0.42
	0.24
	kg N/1000kg animal mass/day

	NEXIPCCdefault
	 Refer to Table 8

	Wsite
	 Refer to Table 8

	TAM
	28
	28
	kg

	Wdefault
	28
	28
	kg

	NEXLT,y
	 Refer to Table 8

	NLT
	 Refer to Table 8

	MS%Bl,j
	100%
	100%
	/

	Fgasm
	40%
	40%
	/

	GWPN2O
	265
	265
	tCO2/t N2O

	CFN20,N-N
	1.57
	1.57
	Conversion Factor N2O-N to N20

	BEN2O,y in 20/01/2021-31/12/2021
	3,238
	tCO2e

	BEN2O,y in 01/01/2022-31/03/2022
	842
	tCO2e

	BEN2O,y
	4,080
	tCO2e



Table 11 The calculation results of baseline emissions
	Period
	BECH4(tCO2e)
	BEN2O,y(tCO2e)
	BEy(tCO2e)

	20/01/2021-31/12/2021
	236,176
	3,238
	239,414 

	01/01/2022-31/03/2022
	61,514
	842
	62,356 

	1st monitoring period
	297,690
	4,080
	301,770 



Project emission
As per section B.6 of the PDD, project emissions can be calculated as follows,

            (Equation 11)
where：
	PEy
	Project emissions in year y

	PEAD,y
	Project emissions associated with the anaerobic digester in year y (t CO2e/yr) 

	PEAer,y
	Project CH4 emissions from aerobic AWMS treatment (t CO2e/yr) 

	PEN2O,y
	Project N2O emissions in year y (t CO2/yr) 

	PEEC/FC,y
	Project emissions from electricity consumption and fossil fuel combustion (t CO2e/yr)



i) Project emissions associated with the anaerobic digester in year y (PEAD,y)
Based on the methodology ACM0010” GHG emission reductions from manure management systems (Version 08.0)”. PEAD,y is determined using the methodological tool “Project and leakage emissions from anaerobic digesters”.

According to the Tool14” Project and leakage emissions from anaerobic digesters (Version 02.0)”, the project emissions associated with the anaerobic digester (PEAD,y) are determined as follows:
              (Equation 12)
where:
	PEAD,y
	Project emissions associated with the anaerobic digester in year y (t CO2e) 

	PEEC,y
	Project emissions from electricity consumption associated with the anaerobic digester in year y (t CO2e) 

	PEFC,y
	Project emissions from fossil fuel consumption associated with the anaerobic digester in year y (t CO2e) 

	PECH4, y
	Project emissions of methane from the anaerobic digester in year y (t CO2e) 

	PEflare,y
	Project emissions from flaring of biogas in year y (t CO2e) 



The biogas generated during the treatment process in this project is captured for power generation and all the electricity generated from this project is used by the AWMSs and 9 swine farms. The electricity generated is not connected to another user or the regional power grid. Unless no electricity generation for this project, the electricity consumption of the project was supplied by the grid company. Since the electricity consumption of the anaerobic digestion system cannot be measured separately from the entire AWMSs, so the Project emissions from electricity consumption associated with the anaerobic digester and that is not related to the anaerobic digester is calculated together.

The project emissions from electricity consumption calculated according to the “Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”, 
              (Equation 13)
Where 
	PEEC,y
	Project emissions from electricity consumption in year y (t CO2e) 

	EGPJ,J,y
	Quantity of electricity consumed by the project electricity consumption source j in year y (MWh/yr) 

	EFEF,j, y
	Emission factor for electricity generation for source j in year y (t CO2/MWh)  

	TDLj,y
	Average technical transmission and distribution losses for providing electricity to source j in year y  



The anaerobic digestion process of this project does not involve the use of fossil fuels, so the project emissions from fossil fuel consumption associated with the anaerobic digester is 0, i.e., PEFC,y=0 

The residual gas is sent to flare system (if any) and project emissions from flaring of biogas (PEflare,y) shall be estimated using the tool 06 “ Project emissions from flaring” (version 04.0).

As described in PDD, project emissions from flaring of biogas (PEflare,y) is determined by the below equation
       (Equation 14)

	Vt,db
	Volumetric flow of the residual gas for flaring in time interval t on a dry basis (m³ dry gas/h) 

	
	Volumetric fraction of greenhouse gas i in the gaseous stream for flaring in a time interval t on a dry basis (m³ gas i/m³ dry gas) 

	
	Density of greenhouse gas i in the gaseous stream in time interval t (kg gas i/m³ gas i) 



Since the gaseous stream is distributed though the same pipeline, and the temperature and pressure of gaseous stream can be stable. Therefore the   of residual gas are same with the biogas produced in the anaerobic digester.

In this monitoring period, all of the biogas generated in the anaerobic process was utilized by the biogas generator to generate electricity.

Determination of project emissions of methane from the anaerobic digester (PECH4,y)
PECH4,y was determined following the step 4 of the applied tool “Project and leakage emissions from anaerobic digesters(Version 02.0)”.Project emissions of methane from the anaerobic digester include emissions during maintenance of the digester, physical leaks through the roof and side walls, and release through safety valves due to excess pressure in the digester. These emissions are calculated using a default emission factor (𝐸𝐹𝐶𝐻4, 𝑑𝑒𝑓𝑎𝑢𝑙𝑡), as follows:
             (Equation 15)
where:
	PECH4, y
	Project emissions of methane from the anaerobic digester in year y (t CO2e) 

	QCH4,y
	Quantity of methane produced in the anaerobic digester in year y (t CH4) 

	EFCH4,default
	Default emission factor for the fraction of CH4 produced that leak from the anaerobic digester (fraction) 

	GWPCH4
	Global warming potential of CH4 (t CO2/tCH4) 



Estimation of various variables and parameters for above equations:
(A) Quantity of methane produced in the anaerobic digester QCH4,y
As per PDD, the biogas is produced and collected from anaerobic digestion process. The flowmeters are installed at the outlet of the anaerobic tanks and the measured on an hourly basis time interval. So the quantity of methane produced in the digester in year y (𝑄𝐶𝐻4,𝑦) is the accumulation of the mass flow of methane in the gaseous stream in an hourly basis time interval. i.e., QCH4,y =

The mass flow of greenhouse gas i (Fi,t) is determined as follows: 
               (Equation 16)
                  (Equation 17)
where:
	Fi,t
	Mass flow of greenhouse gas i in the gaseous stream in time interval t (kg gas/h) 

	Vt,db
	Volumetric flow of the gaseous stream in time interval t on a dry basis (m³ dry gas/h) 

	
	Volumetric fraction of greenhouse gas i in the gaseous stream in a time interval t on a dry basis (m³ gas i/m³ dry gas) 

	
	Density of greenhouse gas i in the gaseous stream in time interval t (kg gas i/m³ gas i) 

	Pt
	Absolute pressure of the gaseous stream in time interval t (Pa) 

	MMi
	Molecular mass of greenhouse gas i (kg/kmol) 

	Ru
	Universal ideal gases constant (Pa.m3/kmol.K) 

	Tt
	Temperature of the gaseous stream in time interval t (K) 



In summary, during this monitoring period, the Project emissions associated with the anaerobic digester in year y (t CO2e) is the sum of Project emissions from electricity consumption and Project emissions of methane from the anaerobic digester in year y (t CO2e). i.e., PEAD,y= PEEC,y + PECH4, y.

ii) Project CH4 emissions from aerobic AWMS treatment (PEAer, y)
IPCC guidelines specify emissions from aerobic lagoons as 0.1 per cent of total methane generating potential of the waste processed, which can be used as a default for all types of aerobic AWMS treatment. 
               (Equation 18)
where:
	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated (fraction) 

	DCH4
	Density of CH4 (t/m3) 

	FAer
	Fraction of volatile solid directed to aerobic system (fraction) 

	LT
	Type of livestock 

	Bo,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	VSLT,y
	Annual volatile solid excretion livestock type LT entering all AWMS on a dry matter weight basis in (kg -dm/animal/yr) 

	NLT
	Annual average number of animals of type LT for the year y (number) as estimated in equation (4) or (5) 

	PEsl,y
	Project CH4 emissions from sludge disposed of in storage pit prior to disposal during the year y (t CO2e/yr) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 



All sludge produced from the aerobic composting will be used for land application, which is calculated as leakage emission, so the PEsl,y=0.

So,       (Equation 19)
where:
	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated (fraction) 

	DCH4
	Density of CH4 (t/m3) 

	FAer
	Fraction of volatile solid directed to aerobic system (fraction) 

	LT
	Type of livestock 

	Bo,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	VSLT,y
	Annual volatile solid excretion livestock type LT entering all AWMS on a dry matter weight basis in (kg -dm/animal/yr) 

	NLT
	Annual average number of animals of type LT for the year y (number) as estimated in equation (4) or (5) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 



iii) Project N2O emissions in year y (PEN2O,y)
          (Equation 20)
where:
	PEN2O,y
	Project N2O emissions in year y (t CO2/yr) 

	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O) 

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28) 

	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/year) 

	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 



             (Equation 21)
where：
	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/yr) 

	EFN2O,D,j
	Direct N2O emission factor for the treatment system j of the manure management system (kg N2O-N/kg N) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%j
	Fraction of manure handled in system j (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



     (Equation 22)
where:
	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 

	EFN2O,ID
	Indirect N2O emission factor for N2O emissions from atmospheric deposition of nitrogen on soils and water surfaces (kgN2O-N/kg NH3-N and NOX-N) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%j
	Fraction of manure handled in system j (fraction) 

	FgasMS,j,LT
	Default values for nitrogen loss due to volatilisation of NH3 and NOX from manure management (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



iV) Project emissions from use of heat and/or electricity (PEelec/heat)
        (Equation 23)
where:
	PEEC,y
	Project emissions from electricity consumption in year y. The project emissions from electricity consumption will be calculated following the latest version of the “Tool to calculate baseline, project and/or leakage emissions from electricity consumption”. In case, the electricity consumption is not measured then the electricity consumption shall be estimated as follows , where CPi,y is the rated capacity (in MW) of electrical equipment i used for the project activity. 

	PEFC,y
	Project emissions from fossil fuel combustion in process j during the year y. The project emissions from fossil fuel combustion will be calculated following the latest version of the “Tool to calculate project or leakage CO2 emissions from fossil fuel combustion”. For this purpose, the processes j in the tool corresponds to all fossil fuel combustion in the AWMS (not including fossil fuels consumed for transportation of feed material and sludge or any other on-site transportation). 



These emissions should only be considered for consumption of electricity or heat that is not related to the anaerobic digester. As described in above, since the electricity consumption that is not related to the anaerobic digester cannot be separated from the total electricity consumption, therefore the emission for consumption of electricity is calculated in PEEC,y.

No fossil fuel is used for this project. Therefore, PEelec/heat=0

Table 12 data for parameter ECPJ,j,y, QCH4,y and FCH4,RG,m
	period
	ECPJ,j,y(MWh)
	QCH4,y(t CH4)
	FCH4,RG,m (t CH4)

	20/01/2021-31/01/2021
	6.26231
	280.00
	0.00

	01/02/2021-28/02/2021
	16.16046
	656.83
	0.00

	01/03/2021-31/03/2021
	16.1535
	729.01
	0.00

	01/04/2021-30/04/2021
	16.14886
	703.61
	0.00

	01/05/2021-31/05/2021
	16.16436
	731.40
	0.00

	01/06/2021-30/06/2021
	16.14563
	706.36
	0.00

	01/07/2021-31/07/2021
	16.1698
	724.47
	0.00

	01/08/2021-31/08/2021
	16.14637
	725.24
	0.00

	01/09/2021-30/09/2021
	16.16606
	699.47
	0.00

	01/10/2021-31/10/2021
	16.14432
	723.54
	0.00

	01/11/2021-30/11/2021
	16.1764
	700.54
	0.00

	01/12/2021-31/12/2021
	16.14725
	731.88
	0.00

	01/01/2022-31/01/2022
	16.16076
	731.24
	0.00

	01/02/2022-28/02/2022
	16.16939
	662.90
	0.00

	01/03/2022-31/03/2022
	16.15244
	716.52
	0.00



Table 13 the calculation result of PEEC,y
	Parameter
	Value
	Unit

	ECPJ,j,y
	Refer to table 12
	MWh

	EFEF,j,y
	0.50885
	tCO2/MWh

	TDLj,y
	20%
	/

	PEEC,y in 20/01/2021-31/12/2021
	113
	tCO2e

	PEEC,y in 01/01/2022-31/03/2022
	30
	tCO2e

	PEEC,y in 1st monitoring period
	143
	tCO2e



Table 14 the calculation result of PECH4,y
	Parameter
	Value
	Unit

	GWPCH4
	28
	tCO2/tCH4

	EFCH4,default
	0.05
	/

	QCH4,y
	Refer to table 12
	t CH4

	PECH4,y in 20/01/2021-31/12/2021
	11,357
	tCO2e

	PECH4,y in 01/01/2022-31/03/2022
	2,955
	tCO2e

	PECH4,y in 1st monitoring period
	14,312
	tCO2e



Table 15 the calculation result of PEflare,y
	Parameter
	Value
	Unit

	GWPCH4
	28
	tCO2/tCH4

	ηflare,m
	0
	/

	FCH4,RG,m
	0
	t CH4

	PEflare,y in 20/01/2021-31/12/2021
	0
	tCO2e

	PEflare,y in 01/01/2022-31/03/2022
	0
	tCO2e

	PEflare,y in 1st monitoring period
	0
	tCO2e



Table 16 calculation of PEAD,y
	Period
	PEEC,y (tCO2e)
	PECH4,y (tCO2e)
	PEflare,y (tCO2e)
	PEAD,y (tCO2e)

	20/01/2021-31/12/2021
	113
	11,357
	0
	11,470

	01/01/2022-31/03/2022
	30
	2,955
	0
	2,985

	1st monitoring period
	143
	14,312
	0
	14,455



Table 17 The calculation result of PEAer,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	GWPCH4
	28
	28
	tCO2/tCH4

	DCH4
	0.00067
	0.00067
	t/m3

	
	0.001
	0.001
	kg N/1000kg animal mass/day

	FAer
	100%
	100%
	/

	1-Rvs,1
	20%
	20%
	/

	B0,LT
	0.29
	0.29
	m3CH4/kg-dm

	NLT
	Refer to Table 8

	VSLT,y
	Refer to Table 8

	MS%j
	100%
	100%
	

	PEAer,y in 20/01/2021-31/12/2021
	81 
	tCO2e

	PEAer,y in 01/01/2022-31/03/2022
	21 
	tCO2e

	PEAer,y in 1st monitoring period
	102 
	tCO2e



Table 18 The calculation result of PEN2O,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	EFN2O,D,j
	0
	0
	kg N2O-N/kg N

	NEXLT,y
	Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	/

	EN2O,D,y  in 20/01/2021-31/12/2021
	0
	kg N2O-N/year

	EN2O,D,y  in 01/01/2022-31/03/2022
	0
	kg N2O-N/year

	EN2O,D,y in the 1st monitoring period
	0
	kg N2O-N/year

	EFN2O,D,j
	0.006
	0.006
	kg N2O-N/kg N

	NEXLT,y
	Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	/

	EN2O,D,y  in 20/01/2021-31/12/2021
	11,683
	kg N2O-N/year

	EN2O,D,y  in 01/01/2022-31/03/2022
	3,039
	kg N2O-N/year

	EN2O,D,y in the 1st monitoring period
	14,722
	kg N2O-N/year

	EFN2O,ID
	0.01
	0.01
	kg N2O-N/kg NH3 and NOX-N

	FgasMS,j,LT
	0.4
	0.4
	/

	NEXLT,y
	Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	%

	GWPN2O
	265
	265
	tCO2/tN2O

	EN2O,ID,y in 20/01/2021-31/12/2021
	7,801
	kg N2O-N/year

	EN2O,ID,y in 01/01/2022-31/03/2022
	2,028
	kg N2O-N/year

	EN2O,ID,y in the 1st monitoring period
	9,829
	kg N2O-N/year

	EFN2O,iD
	0.01
	0.01
	kg N2O/kg N

	Fgasm
	0.45
	0.45
	/

	NEXLT,y
	Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	%

	GWPN2O
	265
	265
	tCO2/tN2O

	EN2O,ID,y in 20/01/2021-31/12/2021
	8,773
	kg N2O-N/year

	EN2O,ID,y in 01/01/2022-31/03/2022
	2,281
	kg N2O-N/year

	EN2O,ID,y in the 1st monitoring period
	11,054
	kg N2O-N/year

	PEN2O,y in 20/01/2021-31/12/2021
	11,767
	tCO2e

	PEN2O,y n 01/01/2022-31/03/2022
	3,059
	tCO2e

	PEN2O,y in the 1st monitoring period
	14,826
	tCO2e



Table 19 Calculation results of project emissions 
	Period
	PEAD,y
(tCO2e)
	PEAer,y
(tCO2e)
	PEN2O,y
(tCO2e)
	PEy
(tCO2e)

	20/01/2021-31/12/2021
	11,470
	81
	11,767
	23,318

	01/01/2022-31/03/2022
	2,985
	21
	3,059
	6,065

	1st monitoring period
	14,455
	102
	14,826
	29,383



Leakage emission
As per section B.6.1 of the PDD, Leakage can be calculated as follows,
            (Equation 24)
Where:
	LEPJ, N2O, y
	Leakage N2O emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	LEBL, N2O, y
	Leakage N2O emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEPJ, CH4, y
	Leakage CH4 emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	LEBL, CH4, y
	Leakage CH4 emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEAD, y
	Leakage emissions associated with the anaerobic digester in year y (t CO2e) 



i) Estimation of leakage N2O emissions released during baseline scenario from land application of the treated manure in year y, LEBL, N2O, y
       (Equation 25)
         (Equation 26)
        (Equation 27)
      (Equation 28)
where:
	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O)

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28)

	LEN2O,land,y
	Leakage N2O emissions from application of manure waste in year y (kg N2O-N/year)

	LEN2O,runoff,y
	Leakage N2O emissions due to leaching and run-off in year y (kg N2O-N/year)

	LEN2O,vol,y
	Leakage N2O emissions due to volatilisation in year y (kg N2O-N/year)

	Fgasm
	Fraction of N lost due to volatilization (fraction) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5) (number) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/year) estimated as described in appendix 2 

	EF1
	Emission factor for N2O emissions from N inputs (kg N2O-N/kg N input) 

	EF5
	Emission factor for N2O emissions from N leaching and runoff in (kg N2O-N/kg N leached and runoff) 

	EF4
	Emission factor for N2O emissions from atmospheric deposition of N on soils and water surfaces, [kg N- N2O/ (kg NH3-N + NOX-N volatilized)] 

	Fleach
	Fraction of all N added to/mineralised in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff (fraction) 

	RN,n
	Nitrogen reduction factor (fraction) 



ii) Estimation of leakage N2O emissions released during project activity from land application of the treated manure in year y, LEPJ, N2O
  (Equation 29)
    (Equation 30)
    (Equation 31)
    (Equation 32)
where:
	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O)

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28)

	LEN2O,land,y
	Leakage N2O emissions from application of manure waste in year y (kg N2O-N/year)

	LEN2O,runoff,y
	Leakage N2O emissions due to leaching and run-off in year y (kg N2O-N/year)

	LEN2O,vol,y
	Leakage N2O emissions due to volatilisation in year y (kg N2O-N/year)

	Fgasm
	Fraction of N lost due to volatilization (fraction) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5) (number) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/year) estimated as described in appendix 2 

	EF1
	Emission factor for N2O emissions from N inputs (kg N2O-N/kg N input) 

	EF5
	Emission factor for N2O emissions from N leaching and runoff in (kg N2O-N/kg N leached and runoff) 

	EF4
	Emission factor for N2O emissions from atmospheric deposition of N on soils and water surfaces, [kg N- N2O/ (kg NH3-N + NOX-N volatilized)] 

	Fleach
	Fraction of all N added to/mineralised in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff (fraction) 

	RN,n
	Nitrogen reduction factor (fraction) 



It is not possible to measure the quantity of manure applied to land in kg manure/yr (QDM) and the nitrogen concentration in kg N/kg manure (NDM) in the manure to estimate the total quantity of nitrogen applied to land. In this case,  does not need to be substituted by. 

iii) Estimation of leakage CH4 emissions from land application of the treated manure
The calculation of methane emissions from land application of manure in the baseline and project cases are estimated as below: 

   (Equation 33)
   (Equation 34)
where:
	LEBL,CH4,y
	Leakage CH4 emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEPJ,CH4,y
	Leakage CH4 emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to sludge being treated 

	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	DCH4
	Density of CH4 (t/m3) 

	B0,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5), expressed (number) 

	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 

	MCFd
	Methane conversion factor (MCF) assumed to be equal to 1 



Table 20 Calculation results of LEBL,CH4,y、LEPJ,CH4,y、LEBL,N2O,y and LEPJ,N2O,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	NLT
	Refer to Table 8

	NEXLT,y
	 Refer to Table 8

	RN,n
	80%
	80%
	/

	EF1
	0.01
	0.01
	kg N2O-N/kg N

	EF5
	0.0075
	0.0075
	kg N2O-N/kg N

	EF4
	0.01
	0.01
	KgN-N2O-N/kg NH3-N+NOX-N

	Fleach
	0.3
	0.3
	/

	Fgasm
	0.2
	0.2
	/

	GWPN2O
	265
	265
	tCO2/t N2O

	LEN2O,land,y in 20/01/2021-31/12/2021
	3,895
	kg N2O-N/year

	LEN2O,land,y in 01/01/2022-31/03/2022
	1,013
	kg N2O-N/year

	LEN2O,land,y in 1st monitoring period
	4,908
	kg N2O-N/year

	LEN2O,runoff,y in 20/01/2021-31/12/2021
	863
	kg N2O-N/year

	LEN2O,runoff,y in 01/01/2022-31/03/2022
	225
	kg N2O-N/year

	LEN2O,runoff,y in 1st monitoring period
	1,088
	kg N2O-N/year

	LEN2O,vol,y in 20/01/2021-31/12/2021
	766
	kg N2O-N/year

	LEN2O,vol,y in 01/01/2022-31/03/2022
	200
	kg N2O-N/year

	LEN2O,vol,y in 1st monitoring period
	966
	kg N2O-N/year

	LEBL,N2O,y in 20/01/2021-31/12/2021
	2,300
	tCO2e

	LEBL,N2O,y in 01/01/2022-31/03/2022
	598
	tCO2e

	LEBL,N2O,y in 1st monitoring period
	2,898
	tCO2e

	NLT
	Refer to Table 8

	NEXLT
	 Refer to Table 8

	RN
	25%
	25%
	-

	RN
	5%
	5%
	-

	EF1
	0.01
	0.01
	kg N2O-N/kg N

	EF5
	0.0075
	0.0075
	kg N2O-N/kg N

	EF4
	0.01
	0.01
	KgN-N2O-N/kg NH3-N+NOX-N

	Fleach
	0.3
	0.3
	/

	Fgasm
	0.2
	0.2
	/

	LEN2O,land,y in 20/01/2021-31/12/2021
	13,886
	kg N2O-N/year

	LEN2O,land,y in 01/01/2022-31/03/2022
	3,611
	kg N2O-N/year

	LEN2O,land,y in 1st monitoring period
	17,497
	kg N2O-N/year

	LEN2O,runoff,y in 20/01/2021-31/12/2021
	3,135
	kg N2O-N/year

	LEN2O,runoff,y in 01/01/2022-31/03/2022
	815
	kg N2O-N/year

	LEN2O,runoff,y in 1st monitoring period
	3,950
	kg N2O-N/year

	LEN2O,vol,y in 20/01/2021-31/12/2021
	2,786
	kg N2O-N/year

	LEN2O,vol,y in 01/01/2022-31/03/2022
	725
	kg N2O-N/year

	LEN2O,vol,y in 1st monitoring period
	3,511
	kg N2O-N/year

	LEPJ,N2O,y in 20/01/2021-31/12/2021
	8,249
	tCO2e

	LEPJ,N2O,y in 01/01/2022-31/03/2022
	2,146
	tCO2e

	LEPJ,N2O,y in 1st monitoring period
	10,395
	tCO2e

	GWPCH4
	28
	28
	tCO2e/t CH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFd
	1
	1
	/

	VSLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	B0,LT
	0.29
	0.29
	m3 CH4/kg-dm

	RVS
	85%
	85%
	/

	MS%j
	100%
	100%
	/

	LEBL,CH4,y in 20/01/2021-31/12/2021
	49,579
	tCO2e

	LEBL,CH4,y in 01/01/2022-31/03/2022
	12,913
	tCO2e

	LEBL,CH4,y in 1st monitoring period
	62,492
	tCO2e

	GWPCH4
	28
	28
	tCO2e/t CH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFd
	1
	1
	/

	VSLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	B0,LT
	0.29
	0.29
	m3 CH4/kg-dm

	RVS
	80%
	80%
	/

	RVS
	20%
	20%
	/

	MS%j
	100%
	100%
	/

	LEPJ,CH4,y in 20/01/2021-31/12/2021
	52,909
	tCO2e

	LEPJ,CH4,y y in 01/01/2022-31/03/2022
	13,781
	tCO2e

	LEPJ,CH4,y1st monitoring period
	66,690
	tCO2e



Table 21 Calculation results of leakage emission
	Period
	LEPJ,CH4,y
(tCO2e)
	LEBL,CH4,y
(tCO2e)
	LEBL,N2O,y (tCO2e)
	LEPJ,N2O,y (tCO2e)
	LEy
(tCO2e)

	20/01/2021-31/12/2021
	52,909
	49,579
	2,300
	8,249
	9,279

	01/01/2022-31/03/2022
	13,781
	12,913
	598
	2,146
	2,416

	1st monitoring period
	66,690
	62,492
	2,898
	10,395
	11,695



In summary, the baseline emission, project emission, leakage emission and emission reductions in this monitoring period are listed below:
	Period
	Baseline emission (tCO2e)
	Project emission (tCO2e)
	Leakage emission (tCO2e)
	Emission reductions (tCO2e)

	20/01/2021-31/12/2021
	239,414 
	23,318 
	9,279 
	206,817

	01/01/2022-31/03/2022
	62,356 
	6,065 
	2,416 
	53,875 

	1st monitoring period
	301,770 
	29,383 
	11,695 
	260,692 



Therefore, the project value or estimation of project situation of SDG13 in this monitoring period is:
Amount of GHGs emission avoided or sequestered from 20/01/2021 to 31/12/2021 is 206,817 tCO2e.
Amount of GHGs emission avoided or sequestered from 01/01/2022 to 31/03/2022 is 53,875 tCO2e.
For the 1st monitoring period from 20/01/2021 to 31/03/2022, Amount of GHGs emission avoided or sequestered is 260,692 tCO2e.

[bookmark: _Toc40962782]Calculation of leakage 
>>
The calculation process of leakage emission in this monitoring period has been described in above Section E.2 of this MR. The calculation result is shown in table 21 of this MR.

[bookmark: _Toc40953319][bookmark: _Toc40953601][bookmark: _Toc40962783][bookmark: _Ref315873988][bookmark: _Toc40962784][bookmark: _Toc40962785]Calculation of net benefits or direct calculation for each SDG Impact

	SDG
	SDG Impact
	Baseline 
estimate
	Project 
estimate
	Net 
benefit

	13
	Amount of GHGs emission avoided or sequestered
	0 tCO2e
	260,692 tCO2e
	260,692 tCO2e

	7
	Total electricity produced
	0MWh
	33,628.11MWh
	33,628.11MWh

	8
	Total number of jobs
	0 full-time jobs created
	18 full-time jobs created (9 females and 19 males)
	18 full-time jobs created (9 females and 9 males)



Furthermore, if the actual methane captured from anaerobic digesters in project activity is lower than (BECH4,y - PEAD,y), then (BECH4,y - PEAD,y) is replaced by actual methane captured QCH4,y.

[bookmark: _Hlk100769809]Total biogas captured through the anaerobic treatment during monitoring period is 26,614,260.38 m3, which equals to 286,233[footnoteRef:14] tCO2e. Baseline methane emission (BECH4,y) is 297,690 tCO2e. Project emissions associated with anaerobic digester is (PEAD,y) is 14,455 tCO2e. Actual methane captured from anaerobic digesters is higher than the difference of BECH4,y and  PEAD,y. Therefore, the equation (BECH4,y - PEAD,y) can be used to calculate emission reduction. [14:  286,233 tCO2e=26,614,260.38m3*0.00063t/m3*60.97%*28tCO2e/tCH4] 


[bookmark: _Toc40962786]Comparison of actual SDG Impacts with estimates in approved PDD 

	SDG
	Values estimated in ex ante calculation of approved PDD 
for this monitoring period
	Actual values achieved during this monitoring period

	13
	319,503[footnoteRef:15] tCO2e [15:  The Yearly total amount estimated emission reduction in PDD is 267,474 tCO2e, so the values estimated emission reduction from 20/01/2021-31/03/2022 is 267,474 tCO2e/365d*436 d=319,503 tCO2e.] 

	260,692 tCO2e

	7
	39,539[footnoteRef:16] MWh electricity produced [16:  The yearly total estimated the electricity produced is 33,100.6MWh, so the value estimated the amount of electricity produced from 20/01/2021-31/03/2022 is 33,100.6MWh /365d*436d=39,539MWh.] 

	33,628.11MWh electricity produced

	8
	18 full-time jobs created (9 females and 9 males)
	18 full-time jobs created (9 females and 9 males)




E.1.1. Explanation of calculation of value estimated ex ante calculation of approved PDD for this monitoring period
>>
According to PDD, the estimated outcomes of SDG 7 for the 1st monitoring period are 39,539 MWh electricity produced annually which is calculated according to the amount of manure produced from the number of animals. while the actual outcomes of SDG 7 are 33,628.11MWh electricity produced in the 1st monitoring period, which is measured by the electric meters. 

For SDG8, total number of jobs created by the project during the 1st monitoring period were determined by the record keeping book and cross-checked with the labor contract. 18 full-time jobs for local people were created (including 9 females and 9 males), which is consistent with the estimated outcomes in the PDD.

The estimated value of the outcomes of SDG 13 for the 1st monitoring period is 319,503 tCO2e, while the actual outcomes of SDG13 is 260,692 tCO2e. The calculation of the estimated and actual value of SDG 13 is based on methodology ACM0010” GHG emission reductions from manure management systems” (version 08.0). 

The mainly difference between the estimated value and actual value for SDG7 and SDG 13 is due to the changes of the number of animals in the swine farm (NLT) and the average animal weight (Wsite).

[bookmark: _Toc40962789]Remarks on increase in achieved SDG Impacts from estimated value in approved PDD
>>
The actual outcomes of SDG 7 are lower than the estimated value in the PDD. The main reason for the difference is that the number of animals in the swine farm. 

The estimated value of the outcomes of SDG 13 for the 1st monitoring period is 319,503 tCO2e, and the actual value is 260,692 tCO2e, which is lower than the estimated value in PDD. The difference between the estimated value and actual values is mainly due to the change of the number of animals in the swine farm and the average animal weight. 

For SDG 8, 18 full-time jobs for local people were created (including 9 females and 9 males) in this monitoring period, which is consistent with the estimated outcomes in the PDD. 

SECTION F. [bookmark: _Toc40962790][bookmark: _Ref47706347][bookmark: _Ref49860694]SAFEGUARDS REPORTING
[bookmark: _Toc40962791]>>
According to the Section D.1 and Appendix 1 in PDD, only one assessment question answered ‘Potentially’ i.e., in case of biogas is not handled properly during the operation period of the project, methane explosion may be caused. Therefore, mitigation measure for safeguarding principles is required and the parameter of Employee Training of biogas safety operation during the operation period shall be monitored, which is described in section D.2 of this MR.

During this monitoring period, no biogas explosion or leakage was happened. The monitoring of this parameters was fully implemented in accordance with the monitoring plan in PDD and the monitoring activities was successful, so there is no need to update the mitigation measures.
SECTION G. [bookmark: _Toc40962792][bookmark: _Ref47706354][bookmark: _Ref49860701]STAKEHOLDER INPUTS AND LEGAL DISPUTES 
[bookmark: _Toc40962793]List all Inputs and Grievances which have been received via the Continuous Input and Grievance Mechanism together with their respective responses/mitigations. 
>>
	Method
	Include all details of Chosen Method (s) so that they may be understood and, where relevant, used by readers.  

	Continuous Input / Grievance Expression Process Book (mandatory)
	A grievance book was put in each swine farm involved in this project. All stakeholders are allowed to record their grievances or comments in the book. The project owner will assign specific person to deal with related issues. When assessing the relevance and appropriateness of the stakeholders’ comments, the project owner will apply a gender lens.

	GS Contact (mandatory)
	help@goldstandard.org 

	Other
	Feedback can be made directly through visiting Shuangbaotai Animal Husbandry Group Co., Ltd. (201, 2nd Floor, Office Building, No. 799, Torch Street, Nanchang High-paying Technology Industrial Development Zone, Nanchang City, Jiangxi Province) or through e-mail snowgirl1984@hotmail.com.



No inputs/grievances received during the 1st monitoring period through all the methods.

Report on any stakeholder mitigations that were agreed to be monitored. 
>>
No inputs/grievances received during the 1st monitoring period; therefore, stakeholder mitigations do not need to be reported.

[bookmark: _Toc40962796]Provide details of any legal contest that has arisen with the project during the monitoring period
>>
No legal contest or dispute has been arisen with the project during the 1st monitoring period.


Revision History

	Version
	Date
	Remarks

	1.1
	14 October 2020
	Hyperlinked section summary to enable quick access to key sections
Improved clarity on Key Project Information
Section for POA monitoring
Forward action request section
Improved Clarity on SDG contribution/SDG Impact term used throughout
Clarity on safeguard reporting
Clarity on design changes
Leakage section added for VER/CER projects
Addition of Comparison of monitored parameters with last monitoring period
Provision of an accompanying Guide to help the user understand detailed rules and requirements

	1.0
	10 July 2017
	Initial adoption
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